HYPER 3D PINBALL INSTALLATION INSTRUCTIONS AND KEY COMMANDS

1.  Place the demo CD into your CD drive.
2.  Switch to your CD drive by typing D: and pressing the <ENTER> key.  (Substitute your CD drive letter if it's not D:)
3.  Type CD\PINBALL and press the <ENTER> key.
4.  Type INSTALL and press the <ENTER> key.
5.  Follow the prompts.
6.  After installing, your video card will be set up.  Follow the prompts.
7.  To run the Hyper 3D Pinball demo, type CD\GAMES\3DPINBAL and press the <ENTER> key.
8.  Type 3DPINBAL and press the <ENTER> key to start the game.


KEY                     FUNCTION
-----                   ---------------
ESC                     pause/options menu
right <SHIFT>           right flipper
left <SHIFT>            left flipper
/                       nudge right
Z                       nudge left
<SPACEBAR>              nudge forward
<RETURN>                pull back plunger
M                       switch to full screen view (where applicable)
3                       switch from full screen to 3D screen (where applicable)
2                       switch from full screen to 2D screen (where applicable)
Q                       quits  (from table selection menu)
