<?xml version="1.0" encoding="UTF-8" ?>
<!DOCTYPE article PUBLIC "-//OASIS//DTD DocBook XML V4.3//EN"
                   "http://www.oasis-open.org/docbook/xml/4.3/docbookx.dtd"
[
<!ENTITY % defs SYSTEM "defs.ent"> %defs;
]>


<!-- lifted from troff+ms+XMan by doclifter -->
<article class="specification" id="xim">

<articleinfo>
   <title>The Input Method Protocol</title>
   <subtitle>X Consortium Standard</subtitle>
   <releaseinfo>X Version 11, Release &fullrelvers;</releaseinfo>
   <releaseinfo>Version 1.0</releaseinfo>
   <authorgroup>
      <author>
         <firstname>Masahiko</firstname><surname>Narita</surname>
         <affiliation><orgname>FUJITSU Limited.</orgname></affiliation>
      </author>
      <author>
         <firstname>Hideki</firstname><surname>Hiura</surname>
         <affiliation><orgname>SunSoft, Inc.</orgname></affiliation>
      </author>
   </authorgroup>
   <copyright><year>1993</year><year>1994</year>
      <holder>FUJITSU LIMITED</holder>
      <holder>Oracle and/or its affiliates</holder>
   </copyright>

<abstract>
<para>
This specifies a protocol between IM library and IM (Input Method) Server for internationalized text input, which is independent from any specific language, any specific input method and the transport layer used in communication between the IM library and the IM Server, and uses a client-server model.  This protocol allows user to use his/her favorite method for all applications within the stand-along distributed environment.
</para>
</abstract>

<legalnotice>
<para>Permission to use, copy and distribute this documentation for any purpose
and without fee is hereby granted, provided that the above copyright notice
and this permission notice appear in all copies.  Fujitsu and Sun Microsystems
make no representation about the suitability for any purpose of the information in this document.
This documentation is provided as is without express implied warranty.
</para>
</legalnotice>

<legalnotice>
<para role="multiLicensing">Copyright © 1993, 1994 X Consortium</para>
<para>Permission is hereby granted, free of charge, to any person obtaining a copy of
this software and associated documentation files (the "Software"), to deal in
the Software without restriction, including without limitation the rights to
use, copy, modify, merge, publish, distribute, sublicense, and/or sell copies
of the Software, and to permit persons to whom the Software is furnished to do
so, subject to the following conditions:
</para>
<para>The above copyright notice and this permission notice shall be included in all
copies or substantial portions of the Software.</para>
<para>THE SOFTWARE IS PROVIDED &ldquo;AS IS&rdquo;, WITHOUT WARRANTY OF ANY KIND, EXPRESS OR
IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY,
FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT. IN NO EVENT SHALL THE X
CONSORTIUM BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN
ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION
WITH THE SOFTWARE OR THE USE OR OTHER DEALINGS IN THE SOFTWARE.
</para>
<para>
Except as contained in this notice, the name of the X Consortium shall not be
used in advertising or otherwise to promote the sale, use or other dealings in
this Software without prior written authorization from the X Consortium.
</para>
<para>X Window System is a trademark of The Open Group.</para>
</legalnotice>

</articleinfo>

<sect1 id="Introduction">
<title>Introduction</title>
<sect2 id="Scope">
<title>Scope</title>
<!-- .XS -->
<!-- (SN Scope -->
<!-- .XE -->
<para>
<!-- .LP -->
The internationalization in the
X Window System
Version 11, Release 5 (X11R5) provides a common API which application
developers can use to create portable internationalized programs and to
adapt them to the requirements of different native languages, local customs,
and character string encodings (this is called "localization").
As one of its internationalization mechanisms X11R5 has defined a functional
interface for internationalized text input, called XIM (X Input Method).
</para>
<para>
<!-- .LP -->
When a client-server model is used with an IM (Input Method) implementation,
a protocol must be established between the client and the server.
However, the protocol used to interface Input Method Servers (IM Servers)
with the Input Method libraries (IM libraries) to which applications are
linked was not addressed in X11R5.
This led application developers to depend on vendor-specific input methods,
decreased the user's choice of available input methods, and made it more
difficult for developers to create portable applications. This paper describes
the Input Method Protocol developed for X11R6 to resolve the above problems
and to address the requirements of existing and future input methods.
</para>
<para>
<!-- .LP -->
The Input Method Protocol is independent from the transport layer used in
communication between the IM library and the IM Server.
Thus, the input method protocol can be built on any inter-process
communication mechanism, such as TCP/IP or the X protocol.
</para>
<para>
In addition, the protocol provides for future extensions such as differing
input model types.
</para>
</sect2>

<sect2 id="Background">
<title>Background</title>
<!-- .XS -->
<!-- (SN Background -->
<!-- .XE -->
<para>
<!-- .LP -->
Text input is much more simple for some languages than
others.  English, for instance, uses an alphabet of a manageable size,
and input consists of pressing the corresponding key on a keyboard,
perhaps in combination with a shift key for capital letters or special
characters.
</para>
<para>
<!-- .LP -->
Some languages have larger alphabets, or modifiers such as accents,
which require the addition of special key combinations in order to enter
text.  These input methods may require "dead-keys" or "compose-keys"
which, when followed by different combinations of key strokes,
generate different characters.
</para>
<para>
<!-- .LP -->
Text input for ideographic languages is much less simple.  In these
languages, characters represent actual objects rather than phonetic
sounds used in pronouncing a word, and the number of characters
in these languages may continue to grow.  In Japanese, for instance, most
text input methods involve entering characters in a phonetic alphabet,
after which the input method searches a dictionary for possible
ideographic equivalents (of which there may be many).  The input method then
presents the candidate characters for the user to choose from.
</para>
<para>
<!-- .LP -->
In Japanese, either Kana (phonetic symbols) or Roman letters are
typed and then a region is selected for conversion to Kanji. Several
Kanji characters may have the same phonetic representation. If that
is the case with the string entered, a menu of characters is presented
and the user must choose the appropriate one. If no choice is necessary
or a preference has been established, the input method does the
substitution directly.
</para>
<para>
<!-- .LP -->
These complicated input methods must present state information (Status Area),
text entry and edit space (Preedit Area), and menu/choice presentations
(Auxiliary Area).  Much of the protocol between the IM library and the IM
Server involves managing these IM areas.
Because of the size and complexity of these input methods, and because
of how widely they vary from one language or locale to another, they are
usually implemented as separate processes which can serve many client
processes on the same computer or network.
</para>
<para>
<!-- .LP -->
</para>
</sect2>
<sect2 id="Input_Method_Styles">
<title>Input Method Styles</title>
<!-- .XS -->
<!-- (SN Input Method Styles -->
<!-- .XE -->
<para>
<!-- .LP -->
X11 internationalization support includes the following four types of
input method:
<!-- .RS -->
</para>

<variablelist>
  <varlistentry>
    <term>- on-the-spot:</term>
    <listitem>
      <para>
The client application is directed by the IM Server to display all
pre-edit data at the site of text insertion.  The client registers
callbacks invoked by the input method during pre-editing.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term>- off-the-spot:</term>
    <listitem>
      <para>
The client application provides display windows for the pre-edit data
to the input method which displays into them directly.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term>- over-the-spot:</term>
    <listitem>
      <para>
The input method displays pre-edit data in a window which it brings up
directly over the text insertion position.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term>- root-window:</term>
    <listitem>
      <para>
The input method displays all pre-edit data in a separate area of the
screen in a window specific to the input method.
      </para>
    </listitem>
  </varlistentry>
</variablelist>

<para>
Client applications must choose from the available input methods
supported by the IM Server and provide the display areas and callbacks
required by the input method.
</para>
</sect2>

</sect1>
<sect1 id="Architecture">
<title>Architecture</title>
<!-- .XS -->
<!-- (SN Architecture -->
<!-- .XE -->
<sect2 id="Implementation_Model">
<title>Implementation Model</title>
<!-- .XS -->
<!-- (SN Implementation Model -->
<!-- .XE -->
<para>
<!-- .LP -->
Within the X Window System environment, the following two typical
architectural models can be used as an input method's implementation
model.
</para>

<variablelist>
  <varlistentry>
    <term>- Client/Server model:</term>
    <listitem>
      <para>
A separate process, the IM Server, processes input and handles preediting,
converting, and committing.  The IM library within the application, acting
as client to the IM Server, simply receives the committed string from the
IM Server.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term>- Library model:</term>
    <listitem>
      <para>
All input is handled by the IM library within the application.  The
event process is closed within the IM library and a separate IM Server
process may not be required.
      </para>
    </listitem>
  </varlistentry>
</variablelist>

<para>
<!-- .LP -->
Most languages which need complex preediting, such as Asian languages,
are implemented using the Client/Server IM model.  Other languages
which need only dead key or compose key processing, such as European
languages, are implemented using the Library model.
</para>
<para>
<!-- .LP -->
In this paper, we discuss mainly the Client/Server IM model and the
protocol used in communication between the IM library (client) and the IM
Server.
</para>
</sect2>

<sect2 id="Structure_of_IM">
<title>Structure of IM</title>
<!-- .XS -->
<!-- (SN Structure of IM -->
<!-- .XE -->
<para>
<!-- .LP -->
When the client connects or disconnects to the IM Server, an open or close
operation occurs between the client and the IM Server.
</para>
<para>
<!-- .LP -->
The IM can be specified at the time of XOpenIM() by setting the locale
of the client and a locale modifier. Since the IM remembers
the locale at the time of creation XOpenIM() can be called
multiple times (with the
setting for the locale and the locale modifier changed) to support
multiple languages.
</para>
<para>
<!-- .LP -->
In addition, the supported IM type can be obtained using XGetIMValues().
</para>
<para>
<!-- .LP -->
The client usually holds multiple input (text) fields. Xlib provides a
value type called the "Input Context" (IC) to manage each individual
input field.  An IC can be created by specifying XIM using XCreateIC(),
and it can be destroyed using XDestroyIC().
</para>
<para>
<!-- .LP -->
The IC can specify the type of IM which is supported by XIM for each
input field, so each input field can handle a different type of IM.
</para>
<para>
<!-- .LP -->
Most importantly information such as the committed string sent from
the IM Server to the client, is exchanged based on each IC.
</para>
<para>
<!-- .LP -->
Since each IC corresponds to an input field, the focused input field
should be announced to the IM Server using XSetICFocus(). (XUnsetICFocus()
can also be used to change the focus.)
</para>
<para>
<!-- .LP -->
</para>
</sect2>
<sect2 id="Event_Handling_Model">
<title>Event Handling Model</title>
<!-- .XS -->
<!-- (SN Event Handling Model -->
<!-- .XE -->
<para>
<!-- .LP -->
Existing input methods support either the FrontEnd method, the BackEnd method,
or both.  This protocol specifically supports the BackEnd method as
the default method, but also supports the FrontEnd method as an optional
IM Server extension.
</para>
<para>
<!-- .LP -->
The difference between the FrontEnd and BackEnd methods is in how
events are delivered to the IM Server.  (Fig. 1) <!-- xref -->
</para>

<sect3 id="BackEnd_Method">
<title>BackEnd Method</title>
<!-- .XS -->
<!-- (SN BackEnd Method -->
<!-- .XE -->
<para>
<!-- .LP -->
In the BackEnd method, client window input events are always delivered
to the IM library, which then passes them to the IM Server.  Events are
handled serially in the order delivered, and therefore there is no
synchronization problem between the IM library and the IM Server.
</para>
<para>
<!-- .LP -->
Using this method, the IM library forwards all KeyPress and KeyRelease
events to the IM Server (as required by the Event Flow Control model
described in
<xref linkend='Event_Flow_Control' xrefstyle='select: title'/>)
and synchronizes with the IM Server (as described in
<xref linkend='Filtering_Events' xrefstyle='select: title'/>).

</para>
</sect3>

<sect3 id="FrontEnd_Method">
<title>FrontEnd Method</title>
<!-- .XS -->
<!-- (SN FrontEnd Method -->
<!-- .XE -->
<para>
<!-- .LP -->
In the FrontEnd method, client window input events are delivered by the
X server directly to both the IM Server and the IM library.  Therefore this
method provides much better interactive performance while preediting
(particularly in cases such as when the IM Server is running locally on
the user's workstation and the client application is running on another
workstation over a relatively slow network).
</para>
<para>
<!-- .LP -->
However, the FrontEnd model may have synchronization problems between
the key events handled in the IM Server and other events handled in the
client, and these problems could possibly cause the loss or duplication
of key events.  For this reason, the BackEnd method is the core method
supported, and the FrontEnd method is made available as an extension for
performance purposes. (Refer to
<xref linkend="common_extensions" xrefstyle='select: title'/>
for more information.)
</para>

<mediaobject  id="flow_of_events">
  <imageobject>
    <imagedata  format="SVG"  fileref="eventflow.svg"/>
  </imageobject>
  <caption>The flow of events</caption>
</mediaobject>

<!--
<para>
Fig.1 The Flow of Events
</para>
-->

</sect3>
</sect2>

<sect2 id='Event_Flow_Control'>
<title>Event Flow Control</title>
<!-- .XS -->
<!-- (SN Event Flow Control -->
<!-- .XE -->
<para>
<!-- .LP -->
This protocol supports two event flow models for communication between the
IM library and the IM Server (Static and Dynamic).
</para>
<para>
<!-- .LP -->
Static Event Flow requires that input events always be sent to the IM
Server from the client.
</para>
<para>
<!-- .LP -->
Dynamic Event Flow, however, requires only that those input events which
need to be processed (converted) be sent to the IM Server from the client.
</para>
<para>
<!-- .LP -->
For instance, in the case of inputing a combination of ASCII characters
and Chinese characters, ASCII characters do not need to be processed in
the IM Server, so their key events do not have to be sent to the IM
Server.  On the other hand, key events necessary for composing Chinese
characters must be sent to the IM Server.
</para>
<para>
<!-- .LP -->
Thus, by adopting the Dynamic Event Flow, the number of requests among the
X Server, the client, and the IM Server is significantly reduced, and the
number of context switches is also reduced, resulting in improved performance.
The IM Server can send
<function>XIM_REGISTER_TRIGGERKEYS </function>
message in order to switch the event flow in the Dynamic Event Flow.
</para>
<para>
<!-- .LP -->
The protocol for this process is described in
<xref linkend='Event_Flow_Control_2' xrefstyle='select: title'/>.
</para>
</sect2>
</sect1>

<sect1 id="Default_Preconnection_Convention">
<title>Default Preconnection Convention</title>
<!-- .XS -->
<!-- (SN Default Preconnection Convention  -->
<!-- .XE -->
<para>
<!-- .LP -->
IM Servers are strongly encouraged to register their symbolic
names as the ATOM names into the IM Server directory property,
<function>XIM_SERVERS,</function>
on the root window of the screen_number 0.
This property can contain a list of ATOMs, and the each ATOM represents
each possible IM Server.
IM Server names are restricted to POSIX Portable Filename Character Set.
To discover if the IM Server is active, see if there is an owner for
the selection with that atom name.  To learn the address of that IM Server,
convert the selection target
<function>TRANSPORT,</function>
which will return a string form of the transport address(es).
To learn the supported locales of that IM Server, convert the selection target
<function>LOCALES,</function>
which will return a set of names of the supported locales in the syntax
X/Open defines.
</para>
<para>
<!-- .LP -->
The basic semantics to determine the IM Server if there are
multiple ATOMs are found in
<function>XIM_SERVERS</function>
property, is first fit if the IM Server name is not given as
a X modifier's category
<function>im.</function>
</para>
<para>
<!-- .LP -->
The address information retrievable from the
<function>TRANSPORT</function>
target is a transport-specific name.
The preregistered formats for transport-specific names are listed in
<xref linkend="transport_list" xrefstyle='select: title'/>.
Additional transport-specific names may be registered with X Consortium.
</para>

<para>
For environments that lack X connections, or for IM Servers which
do not use the X Window System, the preconnection convention with IM Server
may be given outside the X Window system (e.g. using a Name Service).
</para>
</sect1>

<sect1 id="Protocol">
<title>Protocol</title>
<!-- .XS -->
<!-- (SN Protocol -->
<!-- .XE -->
<para>
<!-- .LP -->
The protocol described below uses the bi-directional
synchronous/asynchronous request/reply/error model and is specified
using the same conventions outlined in Section 2 of the core X Window
System protocol [1]:
</para>

<sect2 id="Basic_Requests_Packet_Format">
<title>Basic Requests Packet Format</title>
<!-- .XS -->
<!-- (SN Basic Requests Packet Format -->
<!-- .XE -->
<para>
<!-- .LP -->
This section describes the requests that may be exchanged between the client
and the IM Server.
</para>
<para>
<!-- .LP -->
The basic request packet header format is as follows.
</para>
<literallayout class="monospaced">
          major-opcode:               CARD8
          minor-opcode:               CARD8
          length:                     CARD16
</literallayout>

<para>
The MAJOR-OPCODE specifies which core request or extension package this
packet represents.  If the MAJOR-OPCODE corresponds to a core request,
the MINOR-OPCODE contains 8 bits of request-specific data.
(If the MINOR-OPCODE is not used, it is 0.)
Otherwise, the MAJOR-OPCODE and the MINOR-OPCODE are specified by
<function>XIM_QUERY_EXTENSION</function>
message.  (Refer to 4.7. Query the supported extension protocol list.)
The LENGTH field specifies the number of 4 bytes elements following the
header.  If no additional data is followed by the header, the LENGTH field
will be 0.
</para>
</sect2>

<sect2 id="Data_Types">
<title>Data Types</title>
<!-- .XS -->
<!-- (SN Data Types -->
<!-- .XE -->
<para>
The following data types are used in the core X IM Server protocol:
</para>

<literallayout class="monospaced">
BITMASK16
     CARD16
BITMASK32
     CARD32
PADDING FORMAT
     Where N is some expression, and Pad(N) is the number of bytes needed to round N up to a

          Pad(N) = (4 - (N mod 4)) mod 4

LPCE
  1          A character from the4 X Portable Character Set in Latin Portable
             Character Encoding

STRING
     2     n              length of string in bytes
     n     LISTofLPCE     string
     p                    unused, p=Pad(2+n)

STR
     1     n              length of name in bytes
     n     STRING8        name

XIMATTR
     2     CARD16         attribute ID (*1)
     2     CARD16         type of the value (*2)
     2     n              length of im-attribute
     n     STRING8        im-attribute
     p                    unused, p = Pad(2+n)

The im-attribute argument specifies XIM values such as XNQueryInputStyle.

XICATTR
     2     CARD16         attribute ID (*1)
     2     CARD16         type of the value (*2)
     2     n              length of ic-attribute
     n     STRING8        ic-attribute
     p                    unused, p = Pad(2+n)

(*1) XIMATTR and XICATTR are used during the setup stage and XIMATTRIBUTE and
     XICATTRIBUTE are used after each attribute ID has been recognized by
     the IM Server and the IM library.

(*2) The value types are defined as follows:
</literallayout>
<informaltable id="valuetypes" frame="topbot">
  <?dbfo keep-together="auto" ?>
  <tgroup cols="5" align='left' colsep='0' rowsep='0'>
  <colspec colname="col1" colwidth="0.9*"/>
  <colspec colname="col2" colwidth="3.0*"/>
  <colspec colname="col3" colwidth="3.2*"/>
  <colspec colname="col4" colwidth="2.9*"/>
  <colspec colname="col5" colwidth="2.9*"/>
  <spanspec namest="col3" nameend="col5" spanname="span-horiz" align="center"/>
  <thead>
    <row rowsep='1'>
      <entry>values</entry>
      <entry>data</entry>
      <entry>format</entry>
      <!-- <entry spanname="span-horiz">format</entry> -->
    </row>
  </thead>
  <tbody>
    <row>
      <entry>#0</entry>
      <entry>Separator of NestedList</entry>
      <entry>-----(*3)</entry>
    </row>
    <row>
      <entry>#1</entry>
      <entry>byte data</entry>
      <entry>CARD8</entry>
    </row>
    <row>
      <entry>#2</entry>
      <entry>word data</entry>
      <entry>CARD16</entry>
    </row>
    <row>
      <entry>#3</entry>
      <entry>long data</entry>
      <entry>CARD32</entry>
    </row>
    <row>
      <entry>#4</entry>
      <entry>char data</entry>
      <entry>STRING8</entry>
    </row>
    <row>
      <entry>#5</entry>
      <entry>Window</entry>
      <entry>CARD32</entry>
    </row>
    <row>
      <entry>#10</entry>
      <entry>XIMStyles</entry>
      <entry>2</entry>
      <entry>n</entry>
      <entry>number of XIMStyle list</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry>2</entry>
      <entry></entry>
      <entry>unused</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry>n</entry>
      <entry>CARD32</entry>
      <entry>XIMStyle list</entry>
    </row>
    <row>
      <entry>#11</entry>
      <entry>XRectangle</entry>
      <entry>2</entry>
      <entry>INT16</entry>
      <entry>X</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry>2</entry>
      <entry>INT16</entry>
      <entry>Y</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry>2</entry>
      <entry>CARD16</entry>
      <entry>width</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry>2</entry>
      <entry>CARD16</entry>
      <entry>height</entry>
    </row>
    <row>
      <entry>#12</entry>
      <entry>XPoint</entry>
      <entry>2</entry>
      <entry>INT16</entry>
      <entry>X</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry>2</entry>
      <entry>INT16</entry>
      <entry>Y</entry>
    </row>
    <row>
      <entry>#13</entry>
      <entry>XFontSet</entry>
      <entry>2</entry>
      <entry>n</entry>
      <entry>length of Base font name</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry>n</entry>
      <entry>STRING8</entry>
      <entry>Base font name list</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry>p</entry>
      <entry></entry>
      <entry>unused, p = Pad(2+n)</entry>
    </row>
    <row>
      <entry>#15</entry>
      <entry>XIMHotKeyTriggers</entry>
      <entry>4</entry>
      <entry>n</entry>
      <entry>number of XIMTRIGGERKEY list (*4)</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry>n</entry>
      <entry>XIMTRIGGERKEY</entry>
      <entry>XIMHotkeyTrigger list</entry>
    </row>
    <row>
      <entry></entry>
      <entry></entry>
      <entry>n</entry>
      <entry>XIMHOTKEYSTATE</entry>
      <entry>HotKey processing state</entry>
    </row>
    <row>
      <entry>#17</entry>
      <entry>XIMStringConversion</entry>
      <entry>XIMSTRCONVTEXT</entry>
      <entry></entry>
      <entry></entry>
    </row>
    <row>
      <entry>#18</entry>
      <entry>XIMPreeditState</entry>
      <entry>XIMPREEDITSTATE</entry>
    </row>
    <row>
      <entry>#19</entry>
      <entry>XIMResetState</entry>
      <entry>XIMRESETSTATE</entry>
    </row>
    <row>
      <entry>#x7fff</entry>
      <entry>NestedList</entry>
      <entry>-----</entry>
    </row>
  </tbody>
  </tgroup>
</informaltable>

<literallayout class="monospaced">
(*3)  The IC value for the separator of NestedList is defined as follows,
            #define   XNSeparatorofNestedList   "separatorofNestedList"
      , which is registered in X Consortium and cannot be used for any other purpose.

(*4) LISTofFOO
            A Type name of the form LISTof FOO means a counted list of elements of type FOO.
            The size of the length field may vary (it is not necessarily the same
            size as a FOO), and in some cases, it may be implicit.
XIMTRIGGERKEY
     4     CARD32       keysym
     4     CARD32       modifier
     4     CARD32       modifier mask

ENCODINGINFO
     2     n            length of encoding info
     n     STRING8      encoding info
     p                  unused, p=Pad(2+n)


     1     CARD8        extension major-opcode
     1     CARD8        extension minor-opcode
     2     n            length of extension name
     n     STRING8      extension name
     p                  unused, p = Pad(n)

XIMATTRIBUTE
     2     CARD16       attribute ID
     2     n            value length
     n                  value
     p                  unused, p = Pad(n)

XICATTRIBUTE
     2     CARD16       attribute ID
     2     n            value length
     n                  value
     p                  unused, p = Pad(n)



XIMSTRCONVTEXT
     2    CARD16                      XIMStringConversionFeedback
          #x0000001                   XIMStringConversionLeftEdge
          #x0000002                   XIMStringConversionRightEdge
          #x0000004                   XIMStringConversionTopEdge
          #x0000008                   XIMStringConversionBottomEdge
          #x0000010                   XIMStringConversionConvealed
          #x0000020                   XIMStringConversionWrapped
     2     n                          byte length of the retrieved string
     n     STRING8                    retrieved string
     p                                unused, p = Pad(n)
     2     m                          byte length of feedback array
     2                                unused
     m     LISTofXIMSTRCONVFEEDBACK   feedback array(*1)

(*1)   This field is reserved for future use.

XIMFEEDBACK
     4    CARD32       XIMFeedback
          #x000001     XIMReverse
          #x000002     XIMUnderline
          #x000004     XIMHighlight
          #x000008     XIMPrimary
          #x000010     XIMSecondary
          #x000020     XIMTertiary
          #x000040     XIMVisibleToForward
          #x000080     XIMVisibleToBackward
          #x000100     XIMVisibleCenter

XIMHOTKEYSTATE
     4    CARD32       XIMHotKeyState
          #x0000001    XIMHotKeyStateON
          #x0000002    XIMHotKeyStateOFF

XIMPREEDITSTATE
     4    CARD32       XIMPreeditState
          #x0000001    XIMPreeditEnable
          #x0000002    XIMPreeditDisable

XIMRESETSTATE
     4    CARD32       XIMResetState
          #x0000001    XIMInitialState
          #x0000002    XIMPreserveState
</literallayout>
</sect2>

<sect2 id="Error_Notification">
<title>Error Notification</title>
<!-- .XS -->
<!-- (SN Error Notification -->
<!-- .XE -->
<para>
Both the IM Server and the IM library return
<function>XIM_ERROR</function>
messages instead of the corresponding reply messages if any errors occur
during data processing.
</para>

<para>
At most one error is generated per request. If more than one error condition
is encountered in processing a request, the choice of which error is returned
is implementation-dependent.
</para>

<literallayout class="monospaced">
XIM_ERROR (IM Server &lt;--&gt; IM library)
<!-- .sp 6p -->
          2     CARD16          input-method-ID
          2     CARD16          input-context-ID
          2     BITMASK16       flag (*1)
                #0000           Both Input-Method-ID and Input-Context-ID are invalid
                #0001           Input-Method-ID is valid
                #0002           Input-Context-ID is valid
          2     CARD16          Error Code
                #1              BadAlloc
                #2              BadStyle
                #3              BadClientWindow
                #4              BadFocusWindow
                #5              BadArea
                #6              BadSpotLocation
                #7              BadColormap
                #8              BadAtom
                #9              BadPixel
                #10             BadPixmap
                #11             BadName
                #12             BadCursor
                #13             BadProtocol
                #14             BadForeground
                #15             BadBackground
                #16             LocaleNotSupported
                #999            BadSomething (*2)
          2     n               byte length of error detail.
          2     CARD16          type of error detail (*3)
          n     STRING8         error detail (*4)
          p                     unused, p = Pad(n)

(*1)  Before an IM is created, both Input-Method-ID and
      Input-Context-ID are invalid.
      Before an IC is created, only Input-Method-ID is valid.
      After that, both of Input-Method-ID and Input-Context-ID are valid.

(*2) Unspecific error, for example "language engine died"

(*3) This field is reserved for future use.

(*4) Vendor defined detail error message
</literallayout>
</sect2>

<sect2 id="Connection_Establishment">
<title>Connection Establishment</title>
<!-- .XS -->
<!-- (SN Connection Establishment -->
<!-- .XE -->
<para>
<function>XIM_CONNECT</function>
message requests to establish a connection over a mutually-understood virtual
stream.
</para>

<literallayout class="monospaced">
XIM_CONNECT (IM library -&gt; IM Server)
     1                      byte order
           #x42             MSB first
           #x6c             LSB first
     1                      unused
     2     CARD16           client-major-protocol-version (*1)
     2     CARD16           client-minor-protocol-version (*1)
     2     CARD16           number of client-auth-protocol-names
     n     LISTofSTRING     client-auth-protocol-names

(*1) Specify the version of IM Protocol that the client supports.
</literallayout>

<para>
A client must send
<function>XIM_CONNECT</function>
message as the first message on the connection.
The list specifies the names of authentication protocols the sending
IM Server is willing to perform.
(If the client need not authenticate, the list may be omitted.)
</para>

<para>
<function>XIM_AUTH_REQUIRED </function>
message is used to send the authentication protocol name and protocol-specific
data.
</para>

<literallayout class="monospaced">
XIM_AUTH_REQUIRED (IM library &lt;--&gt; IM Server)

     1     CARD8              auth-protocol-index
     3                        unused
     2     n                  length of authentication data
     2                        unused
     n     &lt;varies&gt;     data
     p                        unused, p = Pad(n)
</literallayout>

<para>
The auth-protocol is specified by an index into the list of names
given in the
<function>XIM_CONNECT</function>
or
<function>XIM_AUTH_SETUP</function>
message. Any protocol-specific data that might be required is also sent.
</para>

<para>
The IM library sends
<function>XIM_AUTH_REPLY</function>
message as the reply to
<function>XIM_AUTH_REQUIRED</function>
message, if the IM Server is authenticated.
</para>

<literallayout class="monospaced">
XIM_AUTH_REPLY (IM library -&gt; IM Server)
     2     n                 length of authentication data
     2                       unused
     2     n                 length of authentication data
     2                       unused
     n     &lt;varies&gt;      data
     p                       unused, p = Pad(n)
</literallayout>

<para>
The auth data is specific to the authentication protocol in use.
</para>
<para>
<!-- .LP -->
<function>XIM_AUTH_NEXT </function>
message requests to send more auth data.
</para>

<literallayout class="monospaced">
XIM_AUTH_NEXT (IM library &lt;--&gt; IM Server)
     2     n                 length of authentication data
     2                       unused
     n     &lt;varies&gt;      data
     p                       unused, p = Pad(n)
</literallayout>
<para>
The auth data is specific to the authentication protocol in use.
</para>

<para>
<!-- .LP -->
The IM Server sends
<function>XIM_AUTH_SETUP</function>
message to authenticate the client.
</para>

<literallayout class="monospaced">
XIM_AUTH_SETUP (IM Server -&gt; IM library)
     2     CARD16           number of client-auth-protocol-names
     2                      unused
     n     LISTofSTRING     server-auth-protocol-names
</literallayout>

<para>
The list specifies the names of authentication protocols the
client is willing to perform.
</para>

<para>
<function>XIM_AUTH_NG</function>
message requests to give up the connection.
</para>

<para>
XIM_AUTH_NG (IM library &lt;--&gt; IM Server)
</para>

<para>
The IM Server sends
<function>XIM_CONNECT_REPLY</function>
message as the reply to
<function>XIM_CONNECT</function>
or
<function>XIM_AUTH_REQUIRED</function>
message.
</para>

<literallayout class="monospaced">
XIM_CONNECT_REPLY (IM Server -&gt; IM library)
     2     CARD16     server-major-protocol-version (*1)
     2     CARD16     server-minor-protocol-version (*1)

(*1) Specify the version of IM Protocol that the IM Server supports.
This document specifies major version one, minor version zero.
</literallayout>

<para>
Here are the state diagrams for the client and the IM Server.
</para>

<para>
State transitions for the client
</para>

<variablelist>
  <varlistentry>
    <term><emphasis remap='I'>init_status</emphasis>:</term>
    <listitem>
      <para>
Use authorization function -&gt; <emphasis remap='I'>client_ask</emphasis>
      </para>
      <para>
Not use authorization function -&gt; <emphasis remap='I'>client_no_check</emphasis>
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>start</emphasis>:</term>
    <listitem>
      <para>
Send <function>XIM_CONNECT</function>
      </para>
      <para>
If <emphasis remap='I'>client_ask</emphasis> -&gt; <emphasis remap='I'>client_wait1</emphasis>
      </para>
      <para>
If <emphasis remap='I'>client_no_check</emphasis>,
client-auth-protocol-names may be omitted -&gt; <emphasis remap='I'>client_wait2</emphasis>
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>client_wait1</emphasis>:</term>
    <listitem>
      <para>
Receive <function>XIM_AUTH_REQUIRED</function>
-&gt; <emphasis remap='I'>client_check</emphasis>
      </para>
      <para>
Receive &lt;other&gt; -&gt; <emphasis remap='I'>client_NG</emphasis>
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>client_check</emphasis>:</term>
    <listitem>
      <para>
If no more auth needed, send <function>XIM_AUTH_REPLY</function>
-&gt; <emphasis remap='I'>client_wait2</emphasis>
      </para>
      <para>
If good auth data, send <function>XIM_AUTH_NEXT</function>
-&gt; <emphasis remap='I'>client_wait1</emphasis>
      </para>
      <para>
If bad auth data, send <function>XIM_AUTH_NG</function>
-&gt; give up on this protocol
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>client_wait2</emphasis>:</term>
    <listitem>
      <para>
Receive <function>XIM_CONNECT_REPLY</function>
-&gt; connect Receive
<function>XIM_AUTH_SETUP </function>
-&gt; <emphasis remap='I'>client_more</emphasis>
      </para>
      <para>
Receive <function>XIM_AUTH_NEXT</function>
-&gt; <emphasis remap='I'>client_more</emphasis>
      </para>
      <para>
Receive <function>XIM_AUTH_NG</function>
-&gt; give up on this protocol
      </para>
      <para>
Receive &lt;other&gt; -&gt; <emphasis remap='I'>client_NG</emphasis>
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>client_more</emphasis>:</term>
    <listitem>
      <para>
Send <function>XIM_AUTH_REQUIRED</function>
-&gt; <emphasis remap='I'>client_wait2</emphasis>
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>client_NG</emphasis>:</term>
    <listitem>
      <para>
Send <function>XIM_AUTH_NG</function>
-&gt; give up on this protocol
      </para>
    </listitem>
  </varlistentry>
</variablelist>

<para>
State transitions for the IM Server
</para>

<variablelist>
  <varlistentry>
    <term><emphasis remap='I'>init_status</emphasis>:</term>
    <listitem>
      <para>
Use authorization function -&gt; <emphasis remap='I'>server_ask</emphasis>
      </para>
      <para>
Not use authorization function -&gt; <emphasis remap='I'>server_no_check</emphasis>
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>start</emphasis>:</term>
    <listitem>
      <para>
Receive <function>XIM_CONNECT</function>
      </para>
      <para>
-&gt; <emphasis remap='I'>start2</emphasis>
Receive &lt;other&gt; -&gt; <emphasis remap='I'>server_NG</emphasis>
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>start2</emphasis>:</term>
    <listitem>
      <para>
If <emphasis remap='I'>client_ask</emphasis>, send
<function>XIM_AUTH_REQUIRED</function>
-&gt; <emphasis remap='I'>server_wait1</emphasis>
      </para>
      <para>
If <emphasis remap='I'>client_no_check</emphasis> and
<emphasis remap='I'>server_ask</emphasis>, send
<function>XIM_AUTH_SETUP</function>
-&gt; <emphasis remap='I'>server_wait2</emphasis>
      </para>
      <para>
If <emphasis remap='I'>client_no_check</emphasis> and
<emphasis remap='I'>server_no_check</emphasis>, send
<function>XIM_CONNECT_REPLY</function>
-&gt; connect
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>server_wait1</emphasis>:</term>
    <listitem>
      <para>
Receive
<function>XIM_AUTH_REPLY</function>
-&gt; <emphasis remap='I'>server2</emphasis>
      </para>
      <para>
Receive
<function>XIM_AUTH_NEXT</function>
-&gt; <emphasis remap='I'>server_more</emphasis>
      </para>
      <para>
Receive &lt;other&gt; -&gt; <emphasis remap='I'>server_NG</emphasis>
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>server_more</emphasis></term>
    <listitem>
      <para>
Send
<function>XIM_AUTH_REQUIRED</function>
-&gt; <emphasis remap='I'>server_wait1</emphasis>
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>server2</emphasis></term>
    <listitem>
      <para>
If <emphasis remap='I'>server_ask</emphasis>, send
<function>XIM_AUTH_SETUP</function>
-&gt; <emphasis remap='I'>server_wait2</emphasis>
      </para>
      <para>
If <emphasis remap='I'>server_no_check</emphasis>, send
<function>XIM_CONNECT_REPLY </function>
-&gt; connect
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>server_wait2</emphasis></term>
    <listitem>
      <para>
Receive
<function>XIM_AUTH_REQUIRED</function>
-&gt; <emphasis remap='I'>server_check</emphasis>
      </para>
      <para>
Receive &lt;other&gt; -&gt; <emphasis remap='I'>server_NG</emphasis>
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>server_check</emphasis></term>
    <listitem>
      <para>
If no more auth data, send
<function>XIM_CONNECT_REPLY</function>
-&gt; connect
      </para>
      <para>
If bad auth data, send
<function>XIM_AUTH_NG</function>
-&gt; give up on this protocol
      </para>
      <para>
If good auth data, send
<function>XIM_AUTH_NEXT</function>
-&gt; <emphasis remap='I'>server_wait2</emphasis>
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term><emphasis remap='I'>server_NG</emphasis></term>
    <listitem>
      <para>
Send
<function>XIM_AUTH_NG</function>
-&gt; give up on this protocol
      </para>
    </listitem>
  </varlistentry>
</variablelist>

<para>
<function>XIM_DISCONNECT </function>
message requests to shutdown the connection over a mutually-understood
virtual stream.
</para>

<para>
XIM_DISCONNECT (IM library -&gt; IM Server)
</para>

<para>
<function>XIM_DISCONNECT</function>
is a synchronous request.  The IM library should wait until it receives
either an
<function>XIM_DISCONNECT_REPLY</function>
packet or an <function>XIM_ERROR</function> packet.
</para>

<para>
XIM_DISCONNECT_REPLY (IM Server -&gt; IM library)
</para>

<para>
<function>XIM_OPEN</function>
requests to establish a logical connection between the IM library and the IM
Server.
</para>

<literallayout class="monospaced">
XIM_OPEN (IM library -&gt; IM Server)
     n     STR     locale name
     p             unused, p = Pad(n)
</literallayout>

<para>
<function>XIM_OPEN</function>
is a synchronous request.  The IM library should wait until receiving
either an <function>XIM_OPEN_REPLY</function>
packet or an <function>XIM_ERROR </function> packet.
</para>

<literallayout class="monospaced">
XIM_OPEN_REPLY (IM Server -&gt; IM library)
     2     CARD16             input-method-ID
     2     n                  byte length of IM attributes supported
     n     LISTofXIMATTR      IM attributes supported
     2     m                  byte length of IC attributes supported
     2     CARD16             unused
     m     LISTofXICATTR      IC attributes supported
</literallayout>

<para>
<function>XIM_OPEN_REPLY</function>
message returns all supported IM and IC attributes in LISTofXIMATTR and
LISTofXICATTR.  These IM and IC attribute IDs are used to reduce the amount
of data which must be transferred via the network. In addition, this
indicates to the IM library what kinds of IM/IC attributes can be used
in this session, and what types of data will be exchanged. This allows
the IM Server provider and application writer to support IM system
enhancements with new IM/IC attributes, without modifying Xlib.
The IC value for the separator of NestedList must be included in the
LISTofXICATTR.
</para>

<para>
<function>XIM_CLOSE </function>
message requests to shutdown the logical connection between the IM library
and the IM Server.
</para>

<literallayout class="monospaced">
XIM_CLOSE (IM library -&gt; IM Server)
     2     CARD16     input-method-ID
     2                unused
</literallayout>

<para>
<function>XIM_CLOSE</function>
is a synchronous request.  The IM library should wait until receiving
either an <function>XIM_CLOSE_REPLY</function>
packet or an <function>XIM_ERROR</function> packet.
</para>

<literallayout class="monospaced">
XIM_CLOSE_REPLY (IM Server -&gt; IM library)
     2     CARD16     input-method-ID
     2                unused
</literallayout>

</sect2>

<sect2 id='Event_Flow_Control_2'>
<title>Event Flow Control</title>
<!-- .XS -->
<!-- (SN Event Flow Control -->
<!-- .XE -->
<para>
<!-- .LP -->
An IM Server must send
<function>XIM_SET_EVENT_MASK </function>
message to the IM library in order for events to be forwarded to the IM
Server, since the IM library initially doesn't forward any events to the
IM Server. In the protocol, the IM Server will specify masks of X events
to be forwarded and which need to be synchronized by the IM library.
</para>

<literallayout class="monospaced">
XIM_SET_EVENT_MASK (IM Server -&gt; IM library)
     2     CARD16        input-method-ID
     2     CARD16        input-context-ID
     4     EVENTMASK     forward-event-mask (*1)
     4     EVENTMASK     synchronous-event-mask (*2)

(*1)  Specify all the events to be forwarded to the IM Server by the IM library.
(*2)  Specify the events to be forwarded with synchronous flag on by the IM library.
</literallayout>

<para>
<function>XIM_SET_EVENT_MASK </function>
is an asynchronous request.  The event masks are valid immediately after
they are set until changed by another
<function>XIM_SET_EVENT_MASK</function>
message.  If input-context-ID is set to zero, the default value of the
input-method-ID will be changed to the event masks specified in the request.
That value will be used for the IC's which have no individual values.
</para>

<para>
Using the Dynamic Event Flow model, an IM Server sends
<function>XIM_REGISTER_TRIGGERKEYS </function>
message to the IM library before sending
<function>XIM_OPEN_REPLY</function>
message.
Or the IM library may suppose that the IM Server uses the Static Event Flow
model.
</para>

<literallayout class="monospaced">
XIM_REGISTER_TRIGGERKEYS (IM Server -&gt; IM library)
<!-- .sp 6p -->
     2     CARD16                  input-method-ID
     2                             unused
     4     n                       byte length of on-keys
     n     LISTofXIMTRIGGERKEY     on-keys list
     4     m                       byte length of off-keys
     m     LISTofXIMTRIGGERKEY     off-keys list
</literallayout>

<para>
<function>XIM_REGISTER_TRIGGERKEYS</function>
is an asynchronous request.
The IM Server notifys the IM library of on-keys and off-keys lists with
this message.
</para>

<para>
The IM library notifys the IM Server with
<function>XIM_TRIGGER_NOTIFY </function>
message that a key event matching either on-keys or off-keys has been occurred.
</para>

<literallayout class="monospaced">
XIM_TRIGGER_NOTIFY (IM library -&gt; IM Server)
     2     CARD16           input-method-ID
     2     CARD16           input-context-ID
     4     CARD32           flag
           #0               on-keys list
           #1               off-keys list
     4     CARD32           index of keys list
     4     EVENTMASK        client-select-event-mask (*1)

(*1)  Specify the events currently selected by the IM library with XSelectInput.

</literallayout>

<para>
<function>XIM_TRIGGER_NOTIFY </function>
is a synchronous request.  The IM library should wait until receiving
either an <function>XIM_TRIGGER_NOTIFY_REPLY</function>
packet or an <function>XIM_ERROR</function> packet.
</para>

<literallayout class="monospaced">
XIM_TRIGGER_NOTIFY_REPLY (IM Server -&gt; IM library)
     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

</sect2>

<sect2 id="Encoding_Negotiation">
<title>Encoding Negotiation</title>
<para>
<function>XIM_ENCODING_NEGOTIATION</function>
message requests to decide which encoding to be sent across the wire.
When the negotiation fails, the fallback default encoding is Portable
Character Encoding.
</para>

<literallayout class="monospaced">
XIM_ENCODING_NEGOTIATION (IM library -&gt; IM Server).sp 6p
     2     CARD16                 input-method-ID
     2     n                      byte length of encodings listed by name
     n     LISTofSTR              list of encodings supported in the IM library.
     p                            unused, p = Pad(n)
     2     m                      byte length of encodings listed by detailed data
     2                            unused
     m     LISTofENCODINGINFO     list of encordings supported in the IM library
</literallayout>

<para>
The IM Server must choose one encoding from the list sent by the IM library.
If index of the encording determined is -1 to indicate that the negotiation
is failed, the fallback default encoding is used.
The message must be issued after sending
<function>XIM_OPEN</function> message via XOpenIM().
The name of encoding may be registered with X Consortium.
</para>

<para>
<function>XIM_ENCODING_NEGOTIATION</function>
is a synchronous request.  The IM library should wait until receiving
either an <function>XIM_ENCODING_NEGOTIATION_REPLY</function>
packet or an <function>XIM_ERROR</function> packet.
</para>


<literallayout class="monospaced">
XIM_ENCODING_NEGOTIATION_REPLY (IM Server -&gt; IM library)
     2     CARD16     input-method-ID
     2     CARD16     category of the encoding determined.
           #0         name
           #1         detailed data
     2     INT16      index of the encoding determined.
     2                unused
</literallayout>

</sect2>

<sect2 id="Query_the_supported_extension_protocol_list">
<title>Query the supported extension protocol list</title>
<para>
<function>XIM_QUERY_EXTENSION</function>
message requests to query the IM extensions supported by the IM Server to
which the client is being connected.
</para>

<literallayout class="monospaced">
XIM_QUERY_EXTENSION (IM library -&gt; IM Server)
     2     CARD16        input-method-ID
     2     n             byte length of extensions supported by the IM library
     n     LISTofSTR     extensions supported by the IM library
     p                   unused, p = Pad(n)
</literallayout>

<para>
An example of a supported extension is FrontEnd.
The message must be issued after sending
<function>XIM_OPEN </function> message via XOpenIM().
</para>

<para>
If n is 0, the IM library queries the IM Server for all extensions.
</para>

<para>
If n is not 0, the IM library queries whether the IM Server supports the
contents specified in the list.
</para>

<para>
If a client uses an extension request without previously having issued a
<function>XIM_QUERY_EXTENSION</function>
message for that extension, the IM Server responds with a
<function>BadProtocol</function>
error.  If the IM Server encounters a request with an unknown MAJOR-OPCODE
or MINOR-OPCODE, it responds with a
<function>BadProtocol</function> error.
</para>

<para>
<function>XIM_QUERY_EXTENSION</function>
is a synchronous request.  The IM library should wait until receiving
either an <function>XIM_QUERY_EXTENSION_REPLY</function>
packet or an <function>XIM_ERROR</function> packet.
</para>

<literallayout class="monospaced">
XIM_QUERY_EXTENSION_REPLY (IM Server -&gt; IM library)
     2     CARD16      input-method-ID
     2     n           byte length of extensions supported by both the IM library and the IM Server
     n     LISTofEXT   list of extensions supported by both the IM library and the IM Server

</literallayout>

<para>
<function>XIM_QUERY_EXTENSION_REPLY</function>
message returns the list of extensions supported by both the IM library and
the IM Server. If the list passed in
<function>XIM_QUERY_EXTENSION</function>
message is NULL, the IM Server returns the full list of extensions supported
by the IM Server.  If the list is not NULL, the IM Server returns the
extensions in the list that are supported by the IM Server.
</para>

<para>
<!-- .LP -->
A zero-length string is not a valid extension name.  The IM library should
disregard any zero-length strings that are returned in the extension list.
The IM library does not use the requests which are not supported by the IM
Server.
</para>

</sect2>

<sect2 id="Setting_IM_Values">
<title>Setting IM Values</title>
<para>
<function>XIM_SET_IM_VALUES </function>
requests to set attributes to the IM.
</para>

<literallayout class="monospaced">
XIM_SET_IM_VALUES (IM library -&gt; IM Server)
     2     CARD16                 input-method-ID
     2     n                      byte length of im-attribute
     n     LISTofXIMATTRIBUTE     im-attributes
</literallayout>

<para>
The im-attributes in
<function>XIM_SET_IM_VALUES</function>
message are specified as a LISTofXIMATTRIBUTE, specifying the attributes
to be set. Attributes other than the ones returned by
<function>XIM_OPEN_REPLY</function>
message should not be specified.
</para>

<para>
<function>XIM_SET_IM_VALUES </function>
is a synchronous request. The IM library should wait until receiving
either an
<function>XIM_SET_IM_VALUES_REPLY</function>
packet or an
<function>XIM_ERROR</function>
packet, because it must receive the error attribute if
<function>XIM_ERROR</function> message is returned.
</para>

<literallayout class="monospaced">
XIM_SET_IM_VALUES_REPLY (IM Server -&gt; IM library)
     2     CARD16     input-method-ID
     2                unused
</literallayout>

<para>
<function>XIM_SET_IM_VALUES_REPLY</function>
message returns the input-method-ID to distinguish replies from multiple IMs.
</para>

</sect2>
<sect2 id="Getting_IM_Values">
<title>Getting IM Values</title>
<para>
<function>XIM_GET_IM_VALUES </function>
requests to query IM values supported by the IM Server currently being
connected.
</para>

<literallayout class="monospaced">
XIM_GET_IM_VALUES (IM library -&gt; IM Server)
     2     CARD16           input-method-ID
     2     n                byte length of im-attribute-id
     n     LISTofCARD16     im-attribute-id
     p                      unused, p=Pad(n)
</literallayout>

<para>
<function>XIM_GET_IM_VALUES</function>
is a synchronous request.  The IM library should wait until it receives
either an
<function>XIM_GET_IM_VALUES_REPLY</function>
packet or an <function>XIM_ERROR</function> packet.
</para>

<literallayout class="monospaced">
XIM_GET_IM_VALUES_REPLY (IM Server -&gt; IM library)
     2     CARD16                 input-method-ID
     2     n                      byte length of im-attributes returned
     n     LISTofXIMATTRIBUTE     im-attributes returned
</literallayout>

<para>
The IM Server returns IM values with
<function>XIM_GET_IM_VALUES_REPLY</function>
message.  The order of the returned im-attribute values corresponds directly
to that of the list passed with the
<function>XIM_GET_IM_VALUES</function> message.
</para>

</sect2>
<sect2 id="Creating_an_IC">
<title>Creating an IC</title>
<para>
<function>XIM_CREATE_IC</function> message requests to create an IC.
</para>

<literallayout class="monospaced">
XIM_CREATE_IC (IM library -&gt; IM Server)
     2     CARD16                 input-method-ID
     2     n                      byte length of ic-attributes
     n     LISTofXICATTRIBUTE     ic-attributes
</literallayout>

<para>
The input-context-id is specified by the IM Server to identify the client
(IC).  (It is not specified by the client in
<function>XIM_CREATE_IC</function>
message.), and it should not be set to zero.
</para>

<para>
<function>XIM_CREATE_IC</function>
is a synchronous request which returns the input-context-ID.
The IM library should wait until it receives either an
<function>XIM_CREATE_IC_REPLY</function>
packet or an
<function>XIM_ERROR</function>
packet.
</para>

<literallayout class="monospaced">
XIM_CREATE_IC_REPLY (IM Server -&gt; IM library)
     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

</sect2>
<sect2 id="Destroying_the_IC">
<title>Destroying the IC</title>
<para>
<function>XIM_DESTROY_IC</function>
message requests to destroy the IC.
</para>

<literallayout class="monospaced">
XIM_DESTROY_IC (IM library -&gt; IM Server)
     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

<para>
<function>XIM_DESTROY_IC </function>
is a synchronous request. The IM library should not free its resources
until it receives an
<function>XIM_DESTROY_IC_REPLY</function>
message because <function>XIM_DESTROY_IC</function>
message may result in Callback packets such as
<function>XIM_PREEDIT_DRAW</function>
and <function>XIM_PREEDIT_DONE.</function>
</para>

<literallayout class="monospaced">
XIM_DESTROY_IC_REPLY (IM Server -&gt; IM library)
     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

</sect2>

<sect2 id="Setting_IC_Values">
<title>Setting IC Values</title>
<para>
<function>XIM_SET_IC_VALUES</function>
messages requests to set attributes to the IC.
</para>


<literallayout class="monospaced">
XIM_SET_IC_VALUES (IM library -&gt; IM Server)
     2     CARD16                 input-method-ID
     2     CARD16                 input-context-ID
     2     n                      byte length of ic-attributes
     2                            unused
     n     LISTofXICATTRIBUTE     ic-attributes
</literallayout>

<para>
The ic-attributes in
<function>XIM_SET_IC_VALUES</function>
message are specified as a LISTofXICATTRIBUTE, specifying the attributes
to be set. Attributes other than the ones returned by
<function>XIM_OPEN_REPLY</function> message should not be specified.
</para>

<para>
<function>XIM_SET_IC_VALUES </function>
is a synchronous request. The IM library should wait until receiving
either an <function>XIM_SET_IC_VALUES_REPLY </function>
packet or an <function>XIM_ERROR</function>
packet, because it must receive the error attribute if
<function>XIM_ERROR</function> message is returned.
</para>


<literallayout class="monospaced">
XIM_SET_IC_VALUES_REPLY (IM Server -&gt; IM library)
<!-- .sp 6p -->
     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

</sect2>
<sect2 id="Getting_IC_Values">
<title>Getting IC Values</title>
<para>
<function>XIM_GET_IC_VALUES</function>
message requests to query IC values supported by the IM Server currently
being connected.
</para>


<literallayout class="monospaced">
XIM_GET_IC_VALUES (IM library -&gt; IM Server)
<!-- .sp 6p -->
     2     CARD16           input-method-ID
     2     CARD16           input-context-ID
     2     n                byte length of ic-attribute-id
     n     LISTofCARD16     ic-attribute-id
     p                      unused, p=Pad(2+n)
</literallayout>

<para>
In LISTofCARD16, the appearance of the ic-attribute-id for the separator
of NestedList shows the end of the heading nested list.
</para>

<para>
<function>XIM_GET_IC_VALUES</function>
is a synchronous request and returns each attribute with its values to
show the correspondence.  The IM library should wait until receiving
either an <function>XIM_GET_IC_VALUES_REPLY</function>
packet or an <function>XIM_ERROR</function> packet.
</para>

<literallayout class="monospaced">
XIM_GET_IC_VALUES_REPLY (IM Server -&gt; IM library)
     2     CARD16                 input-method-ID
     2     CARD16                 input-context-ID
     2     n                      byte length of ic-attribute
     2                            unused
     n     LISTofXICATTRIBUTE     ic-attribute
</literallayout>

</sect2>
<sect2 id="Setting_IC_Focus">
<title>Setting IC Focus</title>
<para>
<function>XIM_SET_IC_FOCUS</function>
message requests to set the focus to the IC.
</para>

<literallayout class="monospaced">
XIM_SET_IC_FOCUS (IM library -&gt; IM Server)
     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

<para>
<function>XIM_SET_IC_FOCUS</function> is an asynchronous request.
</para>

</sect2>
<sect2 id="Unsetting_IC_Focus">
<title>Unsetting IC Focus</title>
<para>
<function>XIM_UNSET_IC_FOCUS</function>
message requests to unset the focus to the focused IC.
</para>

<literallayout class="monospaced">
XIM_UNSET_IC_FOCUS (IM library -&gt; IM Server)
     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

<para>
<function>XIM_UNSET_IC_FOCUS</function>
is an asynchronous request.
</para>

</sect2>

<sect2 id='Filtering_Events'>
<title>Filtering Events</title>
<para>
Event filtering is mainly provided for BackEnd method to allow input method
to capture X events transparently to clients.
</para>

<para>
X Events are forwarded by
<function>XIM_FORWARD_EVENT</function> message.
This message can be operated both synchronously and asynchronously.
If the requester sets the synchronous flag, the receiver must send
<function>XIM_SYNC_REPLY</function>
message back to the requester when all the data processing is done.
</para>
<para>
Protocol flow of BackEnd model
</para>

<para>
With BackEnd method, the protocol flow can be classified into two
methods in terms of synchronization, depending on the synchronous-eventmask
of <function>XIM_SET_EVENT_MASK</function>
message.  One can be called on-demand-synchronous method and another
can be called as full-synchronous method.
</para>

<para>
In on-demand-synchronous method, the IM library always receives
<function>XIM_FORWARD_EVENT</function>
or
<function>XIM_COMMIT</function>
message as a synchronous request. Also, the IM Server needs to synchronously
process the correspondent reply from the IM library and the following
<function>XIM_FORWARD_EVENT</function>
message sent from the IM library when any of the event causes the IM Server
to send
<function>XIM_FORWARD_EVENT</function>
or
<function>XIM_COMMIT</function>
message to the IM library, so that the input service is consistent.  If the
IM library gets the control back from the application after receiving the
synchronous request, the IM library replies for the synchronous request before
processing any of the events. In this time, the IM Server blocks
<function>XIM_FORWARD_EVENT</function>
message which is sent by the IM library, and handles it after receiving the
reply. However, the IM Server handles the other protocols at any time.
</para>

<para>
In full-synchronous method, the IM library always sends
<function>XIM_FORWARD_EVENT</function>
message to the IM Server as a synchronous request. Therefore, the reply to it
from the IM Server will be put between the
<function>XIM_FORWARD_EVENT</function> message and its
<function>XIM_SYNC_REPLY</function> message.  In case of sending
<function>XIM_FORWARD_EVENT</function> or
<function>XIM_COMMIT</function>
message, the IM Server should set the synchronous flag off. Because the
synchronization can be done by the following
<function>XIM_SYNC_REPLY</function> message.
</para>

<para>
Following chart shows one of the simplest protocol flow which only
deals with keyevents for preediting operation.
</para>

<mediaobject  id="sampleprotocolflow">
  <imageobject>
    <imagedata  format="SVG"  fileref="sampleprotocolflow1.svg"/>
  </imageobject>
  <caption>Sample Protocol Flow</caption>
</mediaobject>


<para>
Following chart shows one of the complex protocol flow, which deals
with multiple focus windows and button press event as well as keyevent,
and the focus is moved by the application triggered by both of keyevent
and button press event.
</para>
<mediaobject  id="sampleprotocolflow2">
  <imageobject>
    <imagedata  format="SVG"  fileref="sampleprotocolflow2.svg"/>
  </imageobject>
  <caption>Sample Protocol Flow 2</caption>
</mediaobject>

<literallayout class="monospaced">
XIM_FORWARD_EVENT (IM library &lt;--&gt; IM Server)
     2     CARD16         input-method-ID
     2     CARD16         input-context-ID
     2     BITMASK16      flag
           #0001          synchronous
           #0002          request filtering (*1)
           #0004          request lookupstring (*2)
     2     CARD16         serial number
           XEVENT         X event

(*1)  Indicate the receiver should filter events and possible preedit may be invoked.

(*2)  Indicate the receiver should only do lookup string. The IM Server is expected
to just do a conversion of the key event to the best candidate. This bit may
affect the state of the preedit state (e.g. compose of dead key sequences).
</literallayout>

<para>
XEVENT format is same as the X Protocol event format(xEvent).
As the value of xEvent's sequenceNumber is the bottom of 16 bit of XEvent's
xany.serial, the top of 16 bit is sent by serial number(INT16).
</para>

<para>
<function>XIM_FORWARD_EVENT</function>
message is used for forwarding the events from the IM library to the IM Server
in order for IM to be able to filter the event. On the other hand, this
message is also used for forwarding the events from the IM Server to the IM
library if the event forwarded from the IM library is not filtered.
The IM Server, which receives
<function>XIM_FORWARD_EVENT</function>
message without synchronous bit, should set synchronous bit.
If both "request event filtering" and "request lookupstring" flag are
set, then both filtering and lookup should be done for the same event.
</para>

</sect2>

<sect2 id="Synchronizing_with_the_IM_Server">
<title>Synchronizing with the IM Server</title>

<para>
<function>XIM_SYNC</function>
message requests to synchronize the IM library and the IM Server.
</para>

<literallayout class="monospaced">
XIM_SYNC (IM library &lt;--&gt; IM Server)
     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

<para>
This synchronization can be started either on the IM library side or on the
IM Server side.  The side which receives
<function>XIM_SYNC</function>
message should process all XIM requests before replying. The input-context-ID
is necessary to distinguish the IC with which the IM library and the IM
Server are synchronized.
</para>

<literallayout class="monospaced">
XIM_SYNC_REPLY (IM Server &lt;--&gt; IM library)
     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>



<para>
The side which receives
<function>XIM_FORWARD_EVENT, </function>
<function>XIM_COMMIT</function>
or any other message with synchronous bit, should process all XIM request
before replying, and send
<function>XIM_SYNC_REPLY</function>
message as the reply to the previous message.
</para>

</sect2>

<sect2 id="Sending_a_committed_string">
<title>Sending a committed string</title>
<para>
When the IM Server commits a string, the IM Server sends either the committed
string or list of KeySym, or both, by
<function>XIM_COMMIT</function>
message.
</para>

<literallayout class="monospaced">
XIM_COMMIT (IM Server -&gt; IM library)

     2     CARD16          input-method-ID
     2     CARD16          input-context-ID
     2     BITMASK16       flag
           #0001           synchronous
           #0002           XLookupChars
           #0004           XLookupKeySym
           #0006           XLookupBoth = XLookupChars | XLookupKeySym
</literallayout>

<para>
If flag is XLookupKeySym, the arguments continue as follows:
</para>

<literallayout class="monospaced">
     2                unused
     4     KEYSYM     KeySym
</literallayout>

<para>
If flag is XLookupChars, the arguments continue as follows
</para>

<literallayout class="monospaced">
     2     m              byte length of committed string
     m     LISTofBYTE     committed string
     p                    unused, p = Pad(m)
</literallayout>

<para>
If flag is XLookupBoth, the arguments continue as follows
</para>

<literallayout class="monospaced">
     2                    unused
     4     KEYSYM         KeySym
     2     n              byte length of committed string
     n     LISTofBYTE     committed string
     p                    unused, p = Pad(2+n)
</literallayout>

<para>
The IM Server which receives
<function>XIM_COMMIT</function>
message without synchronous bit should set synchronous bit.
</para>

</sect2>

<sect2 id="Reset_IC">
<title>Reset IC</title>
<para>
<function>XIM_RESET_IC</function>
message requests to reset the status of IC in the IM Server.
</para>

<literallayout class="monospaced">
XIM_RESET_IC (IM library -&gt; IM Server)
     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>


<para>
<function>XIM_RESET_IC</function>
is a synchronous request. The IM library should wait until receiving either an
<function>XIM_RESET_IC_REPLY</function> packet or an
<function>XIM_ERROR</function> packet.
</para>

<literallayout class="monospaced">
XIM_RESET_IC_REPLY (IM Server -&gt; IM library)

     2     CARD16         input-method-ID
     2     CARD16         input-context-ID
     2     n              byte length of preedit string
     n     LISTofBYTE     preedit string
     p                    unused, p = Pad(2+n)
</literallayout>

<para>
<function>XIM_RESET_IC_REPLY </function>
message returns the input-context-ID to distinguish replies from multiple ICs.
</para>

</sect2>
<sect2 id="Callbacks">
<title>Callbacks</title>
<para>
If XIMStyle has XIMPreeditArea or XIMStatusArea set, XIMGeometryCallback
may be used, and if XIMPreeditCallback and/or XIMStatusCallback are set,
corresponding callbacks may be used.
</para>

<para>
Any callback request may be sent from an IM Server to an IM client
asynchronously in response to any request previously sent by the IM client
to the IM Server.
</para>

<para>
When an IM Server needs to send a callback request synchronously with
the request previously sent by an IM client, the IM Server sends it
before replying to the previous request.
</para>

<sect3 id="Negotiating_geometry">
<title>Negotiating geometry</title>
<para>
The IM Server sends
<function>XIM_GEOMETRY </function>
message to start geometry negotiation, if XIMStyle has XIMPreeditArea or
XIMStatusArea set.
</para>


<literallayout class="monospaced">
XIM_GEOMETRY (IM Server -&gt; IM library)

     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

<para>
There is always a single Focus Window, even if some input fields have only
one IC.
</para>

</sect3>

<sect3 id="Converting_a_string">
<title>Converting a string</title>

<literallayout class="monospaced">
XIM_STR_CONVERSION (IM Server -&gt; IM library)

     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
     2     CARD16     XIMStringConversionPosition
     2                unused
     4     CARD32     XIMCaretDirection
           #0         XIMForwardChar
           #1         XIMBackwardChar
           #2         XIMForwardWord
           #3         XIMBackwardWord
           #4         XIMCaretUp
           #5         XIMCaretDown
           #6         XIMNextLine
           #7         XIMCPreviousLine
           #8         XIMLineStart
           #9         XIMLineEnd
           #10        XIMAbsolutePosition
           #11        XIMDontChange
     2     CARD16     factor
     2     CARD16     XIMStringConversionOperation
           #0001      XIMStringConversionSubstitution
           #0002      XIMStringConversionRetrieval
     2     INT16      byte length to multiply the XIMStringConversionType
</literallayout>

<para>
<function>XIM_STR_CONVERSION </function>
message may be used to start the string conversion from the IM Server.
</para>

<literallayout class="monospaced">
XIM_STR_CONVERSION_REPLY (IM library -&gt; IM Server)

     2     CARD16             input-method-ID
     2     CARD16             input-context-ID
     4     CARD32             XIMStringConversionFeedback
           XIMSTRCONVTEXT     XIMStringConversionText
</literallayout>

<para>
<function>XIM_STR_CONVERSION_REPLY </function>
message returns the string to be converted and the feedback information array.
</para>
</sect3>

<sect3 id="Preedit_Callbacks">
<title>Preedit Callbacks</title>

<para>
The IM Server sends
<function>XIM_PREEDIT_START </function>
message to call the XIMPreeditStartCallback function.
</para>

<literallayout class="monospaced">
XIM_PREEDIT_START (IM Server -&gt; IM library)

     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

<para>
The reply to this message must be sent synchronously. The reply forwards
the return value from the callback function to the IM Server.
</para>

<literallayout class="monospaced">
XIM_PREEDIT_START_REPLY (IM library -&gt; IM Server)

     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
     4     INT32     return value
</literallayout>

<para>
<function>XIM_PREEDIT_START_REPLY</function>
message returns the input-context-ID to distinguish replies from multiple
IC's.  The return value contains the return value of the function
XIMPreeditStartCallback.
</para>

<para>
The IM Server sends
<function>XIM_PREEDIT_DRAW </function>
message to call the XIMPreeditDrawCallback function.
</para>

<literallayout class="monospaced">
XIM_PREEDIT_DRAW (IM Server -&gt; IM library)

     2     CARD16                input-method-ID
     2     CARD16                input-context-ID
     4     INT32                 caret
     4     INT32                 chg_first
     4     INT32                 chg_length
     4     BITMASK32             status
           #x0000001             no string
           #x0000002             no feedback
     2     n                     length of preedit string
     n     STRING8               preedit string
     p                           unused, p = Pad(2+n)
     2     m                     byte length of feedback array
     2                           unused
     m     LISTofXIMFEEDBACK     feedback array
</literallayout>

<para>
The fields "caret", "chg_first" and "chg_length" correspond to the
fields of XIMPreeditDrawCallbackStruct.
When the "no string" bit of the status field is set, the text field of
XIMPreeditDrawCallbackStruct is NULL.
When the "no feedback" bit of the status field is set, the text feedback
field of XIMPreeditDrawCallbackStruct is NULL.
When the above bits are not set, "preedit string" contains the preedit
string to be displayed, and the feedback array contains feedback information.
</para>

<para>
The IM Server sends
<function>XIM_PREEDIT_CARET</function>
message to call the PreeditCaretCallback function.
</para>

<literallayout class="monospaced">
XIM_PREEDIT_CARET (IM Server -&gt; IM library)

     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
     4     INT32      position
     4     CARD32     direction
           #0         XIMForwardChar
           #1         XIMBackwardChar
           #2         XIMForwardWord
           #3         XIMBackwardWord
           #4         XIMCaretUp
           #5         XIMCaretDown
           #6         XIMNextLine
           #7         XIMCPreviousLine
           #8         XIMLineStart
           #9         XIMLineEnd
           #10        XIMAbsolutePosition
           #11        XIMDontChange
     4     CARD32     style
           #0         XIMInvisible
           #1         XIMCPrimary
           #2         XIMSecondary
</literallayout>

<para>
Each entry corresponds to a field of XIMPreeditCaretCallbackStruct.
Since this callback sets the caret position, its reply must be sent
synchronously.
</para>

<literallayout class="monospaced">
XIM_PREEDIT_CARET_REPLY (IM library -&gt; IM Server)

     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
     4     CARD32     position
</literallayout>

<para>
The position is the value returned by the callback function after it
has been called.
</para>

<para>
The IM Server sends
<function>XIM_PREEDIT_DONE </function>
message to call the XIMPreeditDoneCallback function.
</para>

<literallayout class="monospaced">
XIM_PREEDIT_DONE (IM Server -&gt; IM library)

     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

</sect3>

<sect3 id="Preedit_state_notify">
<title>Preedit state notify</title>

<literallayout class="monospaced">
XIM_PREEDITSTATE (IM Server -&gt; IM Library)
     2     CARD16        input-method-ID
     2     CARD16        input-context-ID
     4     BITMASK32     XIMPreeditState
           #x0000000     XIMPreeditUnknown
           #x0000001     XIMPreeditEnable
           #x0000002     XIMPreeditDisable
</literallayout>

<para>
<function>XIM_PREEDITSTATE</function>
message is used to call the XIMPreeditStateNotifyCallback function.
</para>

</sect3>

<sect3 id="Status_Callbacks">
<title>Status Callbacks</title>

<para>
The IM Server sends
<function>XIM_STATUS_START </function>
message to call the XIMStatusStartCallback function.
</para>

<literallayout class="monospaced">
XIM_STATUS_START (IM Server -&gt; IM library)

     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

<para>
The IM Server sends
<function>XIM_STATUS_DRAW </function>
message to call the XIMStatusDrawCallback function.
</para>

<literallayout class="monospaced">
XIM_STATUS_DRAW (IM Server -&gt; IM library)

     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
     4     CARD32     type
           #0         XIMTextType
           #1         XIMBitmapType
</literallayout>

<para>
If type is XIMTextType, the arguments continue as follows.
</para>

<literallayout class="monospaced">
     4     BITMASK32            status
           #x0000001            no string
           #x0000002            no feedback
     2     n                    length of status string
     n     STRING8              status string
     p                          unused, p = Pad(2+n)
     2     m                    byte length of feedback array
     2                          unused
     m     LISTofXIMFEEDBACK    feedback array
</literallayout>

<para>
If type is XIMBitmapType, the arguments continue as follows.
</para>

<literallayout class="monospaced">
     4     PIXMAP     pixmap data
</literallayout>

<para>
The field "type" corresponds to the field in XIMStatusDrawCallbackStruct.
</para>

<para>
The IM Server sends
<function>XIM_STATUS_DONE </function>
message to call the XIMStatusDoneCallback function.
</para>

<literallayout class="monospaced">
XIM_STATUS_DONE (IM Server -&gt; IM library)

     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
</literallayout>

</sect3>
</sect2>
</sect1>

<sect1 id="Acknowledgements">
<title>Acknowledgements</title>
<para>
This document represents the culmination of several years of debate and
experiments done under the auspices of the MIT X Consortium i18n working
group.  Although this was a group effort, the author remains responsible
for any errors or omissions.
</para>

<para>
We would like to thank to all members of this group.
And we would like to make special thanks to the following people
(in alphabetical order) for their participation in the IM Protocol
design,
Hector Chan, Takashi Fujiwara, Yoshio Horiuchi, Makoto Inada,
Hiromu Inukai, Mickael Kung, Seiji Kuwari, Franky Ling, Hiroyuki Machida,
Hiroyuki Miyamoto, Frank Rojas, Bob Scheifler, Makiko Shimamura,
Shoji Sugiyama, Hidetoshi Tajima, Masaki Takeuchi, Makoto Wakamatsu,
Masaki Wakao, Nobuyuki Tanaka, Shigeru Yamada, Katsuhisa Yano, Jinsoo Yoon.
</para>

</sect1>

<bibliography>
<title>References</title>
<biblioentry>
  <title>X Window System Protocol Version 11</title>
  <author><firstname>Robert W.</firstname><surname>Scheifler</surname></author>
</biblioentry>

<biblioentry>
  <title>Xlib - C Language X Interface"</title>
  <author><firstname>Robert W.</firstname><surname>Scheifler</surname></author>
</biblioentry>
</bibliography>

<appendix id="common_extensions">
<title>Common Extensions</title>
<para>
Extension opcodes and packet names (e.g.
<function>XIM_EXT_SET_EVENT_MASK</function>
) for additional extensions may be registered with X Consortium.
The following is a commonly well-known extended packet.
</para>

<para>
(1) Extension to manipulate the event handling\fP
</para>

<para>
<!-- .LP -->
<function>XIM_EXT_SET_EVENT_MASK </function>
message specifies the set of event masks that the IM library should manipulate.
</para>

<literallayout class="monospaced">
XIM_EXT_SET_EVENT_MASK (IM Server -&gt; IM library)

     2     CARD16        input-method-ID
     2     CARD16        input-context-ID
     4     EVENTMASK     filter-event-mask (*1)
     4     EVENTMASK     intercept-event-mask (*2)
     4     EVENTMASK     select-event-mask (*3)
     4     EVENTMASK     forward-event-mask (*4)
     4     EVENTMASK     synchronous-event-mask (*5)

     (*1) Specify the events to be neglected by the IM library via XFilterEvent.
     (*2) Specify the events to be deselected by the IM library with XSelectInput.
     (*3) Specify the events to be selected by the IM library with XSelectInput.
     (*4) Specify all the events to be forwarded to the IM Server by the IM library.
     (*5) Specify the events to be forwarded with synchronous flag on by the IM library.
</literallayout>

<para>
<!-- .LP -->
The IM library must reply
<function>XIM_SYNC_REPLY</function>
message to the IM Server. This request is valid after the ic is created.
</para>

<para>
(2) Extension for improvement of performance.
</para>
<para>
The following requests may be used for improvement of performance.
</para>

<para>
<function>XIM_EXT_FORWARD_KEYEVENT</function>
message may be used instead of
<function>XIM_FORWARD_EVENT</function>
message.
</para>

<literallayout class="monospaced">
XIM_EXT_FORWARD_KEYEVENT (IM Server &lt;--&gt; IM library)
     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
     2     BITMASK16     flag
          #0001     synchronous
     2     CARD16     sequence number
     1     BYTE     xEvent.u.u.type
     1     BYTE     keycode
     2     CARD16     state
     4     CARD32     time
     4     CARD32     window
</literallayout>

<para>
<function>XIM_EXT_MOVE</function>
message may be used to change the spot location instead of
<function></function>
XIM_SET_IC_VALUES
message.
It is effective only if the client specified XIMPreeditPosition.
</para>


<literallayout class="monospaced">
XIM_EXT_MOVE (IM library -&gt; IM Server)

     2     CARD16     input-method-ID
     2     CARD16     input-context-ID
     2     INT16     X
     2     INT16     Y
</literallayout>

<para>
<function>XIM_EXT_MOVE</function>
message is a asynchronous request.
</para>

</appendix>
<appendix id="transport_list">
<title>Transport List</title>

<para>
The list of transport specific IM Server address format registered
</para>

<para>
The following format represents the ATOM contained in
<function>XIM_SERVERS</function>
property and the string returned from the request converting
selection target LOCALES and TRANSPORT.
</para>
<literallayout class="monospaced">
     "{<emphasis remap='I'>category</emphasis>=[<emphasis remap='I'>value</emphasis>,...]}..."
</literallayout>
<para>
The following categories are currently registered.
</para>

<literallayout class="monospaced">
<function>server</function>;: IM Server name (used for XIM_SERVERS)
<function>locale</function>;: XPG4 locale name (LOCALES)
<function>transport</function>;: transport-specific name (TRANSPORT)
</literallayout>

<para>
The preregistered formats for transport-specific names are as follows:
</para>

<para>
<function>TCP/IP Names</function>
</para>

<para>
The following syntax should be used for system internal domain names:
</para>
<literallayout class="monospaced">
&lt;<emphasis remap='I'>local name</emphasis>&gt;  ::= "local/"&lt;<emphasis remap='I'>hostname</emphasis>&gt;":"&lt;<emphasis remap='I'>pathname</emphasis>&gt;
</literallayout>
<para>
Where &lt;<emphasis remap='I'>pathname</emphasis>&gt; is a path name of socket address.
</para>

<para>
IM Server's name should be set to &lt;<emphasis remap='I'>pathname</emphasis>&gt; to run multiple IM Server
at the same time
</para>

<para>
The following syntax should be used for Internet domain names:
</para>
<literallayout class="monospaced">
&lt;<emphasis remap='I'>TCP name</emphasis>&gt;  ::=  "tcp/"&lt;<emphasis remap='I'>hostname</emphasis>&gt;":"&lt;<emphasis remap='I'>ipportnumber</emphasis>&gt;
</literallayout>
<para>
where &lt;<emphasis remap='I'>hostname</emphasis>&gt; is either symbolic (such as expo.lcs.mit.edu) or
numeric decimal (such as 18.30.0.212).  The &lt;<emphasis remap='I'>ipportnumber</emphasis>&gt; is the
port on which the IM Server is listening for connections.
For example:
</para>
<literallayout class="monospaced">
tcp/expo.lcs.mit.edu:8012
tcp/18.30.0.212:7890
</literallayout>

<para>
<function>DECnet Names</function>
</para>

<para>
The following syntax should be used for DECnet names:
</para>
<literallayout class="monospaced">
&lt;<emphasis remap='I'>DECnet name</emphasis>&gt;  ::=  "decnet/"&lt;<emphasis remap='I'>nodename</emphasis>&gt;"::IMSERVER$"&lt;<emphasis remap='I'>objname</emphasis>&gt;
</literallayout>
<para>
where &lt;<emphasis remap='I'>nodename</emphasis>&gt; is either
symbolic (such as SRVNOD) or the numeric
decimal form of the DECnet address (such as 44.70).
The &lt;<emphasis remap='I'>objname</emphasis>&gt;
is normal, case-insensitive DECnet object name. For example:
</para>

<literallayout class="monospaced">
DECNET/SRVNOD::IMSERVER$DEFAULT
decnet/44.70::IMSERVER$other
</literallayout>

<para>
<function>X Names</function>
</para>

<para>
The following syntax should be used for X names:
</para>
<literallayout class="monospaced">
&lt;<emphasis remap='I'>X name</emphasis>&gt;  ::=  "X/"
</literallayout>

<para>
If a given category has multiple values, the value is evaluated in order of
setting.
</para>

</appendix>
<appendix id="protocol_number">
<title>Protocol Number</title>

<para>
<function>Major Protocol number</function>
</para>

<literallayout class="monospaced">
XIM_CONNECT                                  #001
XIM_CONNECT_REPLY                            #002
XIM_DISCONNECT                               #003
XIM_DISCONNECT_REPLY                         #004

XIM_AUTH_REQUIRED                            #010
XIM_AUTH_REPLY                               #011
XIM_AUTH_NEXT                                #012
XIM_AUTH_SETUP                               #013
XIM_AUTH_NG                                  #014

XIM_ERROR                                    #020

XIM_OPEN                                     #030
XIM_OPEN_REPLY                               #031
XIM_CLOSE                                    #032
XIM_CLOSE_REPLY                              #033
XIM_REGISTER_TRIGGERKEYS                     #034
XIM_TRIGGER_NOTIFY                           #035
XIM_TRIGGER_NOTIFY_REPLY                     #036
XIM_SET_EVENT_MASK                           #037
XIM_ENCODING_NEGOTIATION                     #038
XIM_ENCODING_NEGOTIATION_REPLY               #039
XIM_QUERY_EXTENSION                          #040
XIM_QUERY_EXTENSION_REPLY                    #041
XIM_SET_IM_VALUES                            #042
XIM_SET_IM_VALUES_REPLY                      #043
XIM_GET_IM_VALUES                            #044
XIM_GET_IM_VALUES_REPLY                      #045

XIM_CREATE_IC                                #050
XIM_CREATE_IC_REPLY                          #051
XIM_DESTROY_IC                               #052
XIM_DESTROY_IC_REPLY                         #053
XIM_SET_IC_VALUES                            #054
XIM_SET_IC_VALUES_REPLY                      #055
XIM_GET_IC_VALUES                            #056
XIM_GET_IC_VALUES_REPLY                      #057
XIM_SET_IC_FOCUS                             #058
XIM_UNSET_IC_FOCUS                           #059
XIM_FORWARD_EVENT                            #060
XIM_SYNC                                     #061
XIM_SYNC_REPLY                               #062
XIM_COMMIT                                   #063
XIM_RESET_IC                                 #064
XIM_RESET_IC_REPLY                           #065

XIM_GEOMETRY                                 #070
XIM_STR_CONVERSION                           #071
XIM_STR_CONVERSION_REPLY                     #072
XIM_PREEDIT_START                            #073
XIM_PREEDIT_START_REPLY                      #074
XIM_PREEDIT_DRAW                             #075
XIM_PREEDIT_CARET                            #076
XIM_PREEDIT_CARET_REPLY                      #077
XIM_PREEDIT_DONE                             #078
XIM_STATUS_START                             #079
XIM_STATUS_DRAW                              #080
XIM_STATUS_DONE                              #081
XIM_PREEDITSTATE                             #082

(*) The IM Server's extension protocol number should be more than #128.
</literallayout>
</appendix>

<appendix id="implementation_tips">

<title>Implementation Tips</title>
<para>
(1) FrontEnd Method
</para>

<para>
FrontEnd method is recognized as a performance acceleration by the
trade off of the variety of the reliability.
</para>

<para>
In order to use the FrontEnd method, the IM library must query the IM
Server to see if the FrontEnd extension is available.  The query is
made by using the
<function>XIM_QUERY_EXTENSION</function>
message. The IM Server may send
<function>XIM_EXT_SET_EVENT_MASK</function>
message with intercept-event-mask, forward-event-mask, and
synchronous-event-mask values set after replying
<function>XIM_QUERY_EXTENSION_REPLY</function>
message.
</para>

<para>
FrontEnd method can be implemented in a couple of ways depending on
how the IM Server utilize
<function>XIM_EXT_SET_EVENT_MASK</function>
message.
</para>

<para>
One approach is to update both of the input mask and the filter-event-mask
depending on the preeidting state. The sample protocol sequence using the
static event flow is as follows:
</para>

<mediaobject  id="staticflow">
  <imageobject>
    <imagedata  scale="75" format="SVG"  fileref="staticflow.svg"/>
  </imageobject>
  <caption>The flow of events</caption>
</mediaobject>

<para>
To pursuit a maximum performance regardless of the preediting mode,
the IM Server may use the dynamic event flow with the following
sample protocol sequence.
</para>

<mediaobject  id="dynamicflow">
  <imageobject>
    <imagedata  scale="75" format="SVG"  fileref="dynamicflow.svg"/>
  </imageobject>
  <caption>The flow of events</caption>
</mediaobject>

<para>
This method can reduce the XIM protocol traffic dramatically
by updating intercept-event-mask and select-event-mask accordingly.
The tradeoff of this performance improvement is that the key
events may be lost or disordered in some particular situation, such as
when the user types the keyboard in following sequence really fast:
</para>

<para>
&lt;preediting on key&gt;"some strings"&lt;preediting off
key&gt;"another string"
</para>

<para>
Since this method requires the input mask updates to the both the IM Server
and Xlib when turning on and off the preediting, and there is a time lag
till the requests take effect when two client issues the input mask updates
simultaneously.
</para>

<para>
Another approach of the FrontEnd method is to update the filter-event-mask
depending on the preediting state and not to update the input mask.
The IM Server must register both of the preediting on key list and off key
list by
<function>XIM_REGISTER_TRIGGERKEYS</function>
message.
In this method, Both the IM Server and the IM client select the same
events on the same client's window, so that the events are delivered
to both of the IM Server and the client. The preediting on and off
states are expressed by whether the key events are filtered or not.
The sample protocol sequence are as follows:
</para>

<para>
&lt;&lt;Using static event flow&gt;&gt;
</para>

<mediaobject  id="staticflowsampleseq">
  <imageobject>
    <imagedata  scale="75" format="SVG"  fileref="staticflowsampleseq.svg"/>
  </imageobject>
  <caption>The flow of events</caption>
</mediaobject>

<para>
&lt;&lt;Using the dynamic event flow&gt;&gt;
</para>

<mediaobject  id="dynamicflowsampleseq">
  <imageobject>
    <imagedata  scale="75" format="SVG"  fileref="dynamicflowsampleseq.svg"/>
  </imageobject>
  <caption>The flow of events</caption>
</mediaobject>

<para>
This method does not have the problem of the time lag when going across
the preediting on and off mode, however, the amount of the performance
acceleration is not as good as the method described above.
</para>

<para>
In general, the FrontEnd method requires some synchronization to some
of the X protocols, such as the ChangeWindowAttribute protocol for the
event mask change or the GrabKey protocol, since it relies on the X's
principal event dispatching mechanism. Any X protocol bindings do not
consider the synchronization might cause some mis-synchronization
between the IM clients and the IM Server.
</para>

<para>
(2) Transport Layer
</para>

<para>
The Xlib XIM implementation is layered into three functions, a protocol
layer, an interface layer and a transport layer. The purpose of this
layering is to make the protocol independent of transport implementation.
Each function of these layers are:
</para>

<variablelist>
  <varlistentry>
    <term>The protocol layer</term>
    <listitem>
      <para>
implements overall function of XIM and calls the interface layer
functions when it needs to communicate to IM Server.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term>The interface layer</term>
    <listitem>
      <para>
separates the implementation of the transport layer from the protocol
layer, in other words, it provides implementation independent hook for
the transport layer functions.
      </para>
    </listitem>
  </varlistentry>
  <varlistentry>
    <term>The transport layer</term>
    <listitem>
      <para>
handles actual data communication with IM Server. It is done by a set
of several functions named transporters.
      </para>
    </listitem>
  </varlistentry>
</variablelist>

<para>
The interface layer and the transport layer make various communication
channels usable such as X Protocol, TCP/IP, DECnet or STREAM.
The following is a sample implementation for the transporter using
the X connection.
Refer to "xtrans" for the transporter using Socket Transport. <!-- xref ?-->
</para>

<para>
At the beginning of the X Transport connection for the XIM transport
mechanism, two different windows must be created either in an Xlib XIM
or in an IM Server, with which the Xlib and the IM Server exchange the
XIM transports by using the ClientMessage events and Window Properties.
In the following, the window created by the Xlib is referred as the
"client communication window", and on the other hand, the window created
by the IM Server is referred as the "IMS communication window".
</para>

<para>
Connection
</para>

<para>
In order to establish a connection, a communication window is created.
A ClientMessage in the following event's format is sent to the owner
window of XIM_SERVER selection, which the IM Server has created.
</para>

<para>
Refer to "The Input Method Protocol" for the XIM_SERVER atom. <!-- xref -->
</para>

<table frame="topbot" id="clientmessage_sent_to_the_ims_window">
  <?dbfo keep-together="always" ?>
  <title>The ClientMessage sent to the IMS window.</title>
  <tgroup cols="3" align='left' colsep='0' rowsep='0'>
  <colspec colname="col1" colwidth="1.0*"/>
  <colspec colname="col2" colwidth="1.0*" colsep="1"/>
  <colspec colname="col3" colwidth="3.5*"/>
  <spanspec namest="col1" nameend="col2" spanname="span-horiz" align="center"/>
  <thead>
    <row rowsep='1'>
      <entry spanname="span-horiz" colsep='1'>Structure Member</entry>
      <entry>Contents</entry>
    </row>
  </thead>
  <tbody>
    <row>
      <entry>int</entry>
      <entry>type</entry>
      <entry>ClientMessage</entry>
    </row>
    <row>
      <entry>u_long</entry>
      <entry>serial</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Bool</entry>
      <entry>send_event</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Display</entry>
      <entry>*display</entry>
      <entry>The display to which connects</entry>
    </row>
    <row>
      <entry>Window</entry>
      <entry>window</entry>
      <entry>IMS Window ID</entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>message_type</entry>
      <entry>XInternAtom(display, "_XIM_XCONNECT", False)</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>format</entry>
      <entry>32</entry>
    </row>
    <row>
      <entry>long</entry>
      <entry>data.l[0]</entry>
      <entry>client communication window ID</entry>
    </row>
    <row>
      <entry>long</entry>
      <entry>data.l[1]</entry>
      <entry>client-major-transport-version (*1)</entry>
    </row>
    <row>
      <entry>long</entry>
      <entry>data.l[2]</entry>
      <entry>client-major-transport-version (*1)</entry>
    </row>
  </tbody>
  </tgroup>
</table>

<para>
In order to establish the connection (to notify the IM Server communication
window), the IM Server sends a ClientMessage in the following event's
format to the client communication window.
</para>

<table frame="topbot" id="clientmessage_sent_by_the_im_server">
  <?dbfo keep-together="always" ?>
  <title>The ClientMessage sent by the IM Server.</title>
  <tgroup cols="3" align='left' colsep='0' rowsep='0'>
  <colspec colname="col1" colwidth="1.0*"/>
  <colspec colname="col2" colwidth="1.0*" colsep="1"/>
  <colspec colname="col3" colwidth="3.5*"/>
  <spanspec namest="col1" nameend="col2" spanname="span-horiz" align="center"/>
  <thead>
    <row rowsep='1'>
      <entry spanname="span-horiz" colsep='1'>Structure Member</entry>
      <entry>Contents</entry>
    </row>
  </thead>
  <tbody>
    <row>
      <entry>int</entry>
      <entry>type</entry>
      <entry>ClientMessage</entry>
    </row>
    <row>
      <entry>u_long</entry>
      <entry>serial</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Bool</entry>
      <entry>send_event</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Display</entry>
      <entry>*display</entry>
      <entry>The display to which connects</entry>
    </row>
    <row>
      <entry>Window</entry>
      <entry>window</entry>
      <entry>client communication window ID</entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>message_type</entry>
      <entry>XInternAtom(display, "_XIM_XCONNECT", False)</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>format</entry>
      <entry>32</entry>
    </row>
    <row>
      <entry>long</entry>
      <entry>data.l[0]</entry>
      <entry>IMS communication window ID</entry>
    </row>
    <row>
      <entry>long</entry>
      <entry>data.l[1]</entry>
      <entry>server-major-transport-version (*1)</entry>
    </row>
    <row>
      <entry>long</entry>
      <entry>data.l[2]</entry>
      <entry>server-minor-transport-version (*1)</entry>
    </row>
    <row>
      <entry>long</entry>
      <entry>data.l[3]</entry>
      <entry>dividing size between ClientMessage and Property (*2)</entry>
    </row>
  </tbody>
  </tgroup>
</table>

<para>
(*1) major/minor-transport-version
</para>
<para>
The read/write method is decided by the combination of
major/minor-transport-version, as follows:
</para>


<table frame="all" id="readwrite_method_and_the_majorminor_transport_version">
  <?dbfo keep-together="always" ?>
  <title>The read/write method and the major/minor-transport-version</title>
  <tgroup cols="3" align='left' colsep='1' rowsep='1'>
  <colspec colname="col1" colwidth="1.0*"/>
  <colspec colname="col2" colwidth="1.0*"/>
  <colspec colname="col3" colwidth="3.0*"/>
  <spanspec namest="col1" nameend="col2" spanname="span-horiz" align="center"/>
  <thead>
    <row>
      <entry spanname="span-horiz" colsep='1'>Transport-version</entry>
      <entry>read/write</entry>
    </row>
    <row>
      <entry>major</entry>
      <entry>minor</entry>
      <entry></entry>
    </row>
  </thead>
  <tbody>
    <row>
      <entry morerows="2">0</entry>
      <entry>0</entry>
      <entry>only-CM &amp; Property-with-CM</entry>
    </row>
    <row>
      <entry>1</entry>
      <entry>only-CM &amp; multi-CM</entry>
    </row>
    <row rowsep="1">
      <entry>2</entry>
      <entry>only-CM &amp; multi-CM &amp; Property-with-CM</entry>
    </row>
    <row rowsep="1">
      <entry>1</entry>
      <entry>0</entry>
      <entry>PropertyNotify</entry>
    </row>
    <row>
      <entry morerows="1">2</entry>
      <entry>0</entry>
      <entry>only-CM &amp; PropertyNotify</entry>
    </row>
    <row>
      <entry>1</entry>
      <entry>only-CM &amp; multi-CM &amp; PropertyNotify</entry>
    </row>
  </tbody>
  </tgroup>
</table>

<literallayout class="monospaced">
only-CM            :    data is sent via a ClientMessage
multi-CM           :    data is sent via multiple ClientMessages
Property-with-CM   :    data is written in Property, and its Atom
                        is send via ClientMessage
PropertyNotify     :    data is written in Property, and its Atom
                        is send via PropertyNotify

</literallayout>

<para>
The method to decide major/minor-transport-version is as follows:
</para>

<itemizedlist>
  <listitem>
    <para>
The client sends 0 as major/minor-transport-version to the IM Server.
The client must support all methods in Table D-3.
The client may send another number as major/minor-transport-version to
use other method than the above in the future.
    </para>
  </listitem>
  <listitem>
    <para>
The IM Server sends its major/minor-transport-version number to
the client. The client sends data using the method specified by the
IM Server.
    </para>
  </listitem>
  <listitem>
    <para>
If major/minor-transport-version number is not available, it is regarded
as 0.
<!-- .RE -->
    </para>
  </listitem>
</itemizedlist>

<para>
(*2) dividing size between ClientMessage and Property
</para>

<para>
If data is sent via both of multi-CM and Property, specify the dividing
size between ClientMessage and Property. The data, which is smaller than
this size, is sent via multi-CM (or only-CM), and the data, which is
lager than this size, is sent via Property.
</para>

<para>
<emphasis role="bold">read/write</emphasis>
</para>

<para>
The data is transferred via either ClientMessage or Window Property in
the X Window System.
</para>

<para>
Format for the data from the Client to the IM Server
</para>

<para>
ClientMessage
</para>

<para>
If data is sent via ClientMessage event, the format is as follows:
</para>


<table frame="topbot" id="clientmessage_events_format_first_or_middle">
  <?dbfo keep-together="always" ?>
<title>The ClientMessage event's format (first or middle)</title>
  <tgroup cols="3" align='left' colsep='0' rowsep='0'>
  <colspec colname="col1" colwidth="1.0*"/>
  <colspec colname="col2" colwidth="1.0*" colsep="1"/>
  <colspec colname="col3" colwidth="3.5*"/>
  <spanspec namest="col1" nameend="col2" spanname="span-horiz" align="center"/>
  <thead>
    <row rowsep='1'>
      <entry spanname="span-horiz" colsep='1'>Structure Member</entry>
      <entry>Contents</entry>
    </row>
  </thead>
  <tbody>
    <row>
      <entry>int</entry>
      <entry>type</entry>
      <entry>ClientMessage</entry>
    </row>
    <row>
      <entry>u_long</entry>
      <entry>serial</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Bool</entry>
      <entry>send_event</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Display</entry>
      <entry>*display</entry>
      <entry>The display to which connects</entry>
    </row>
    <row>
      <entry>Window</entry>
      <entry>window</entry>
      <entry>IMS communication window ID</entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>message_type</entry>
      <entry>XInternAtom(display, "_XIM_MOREDATA", False)</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>format</entry>
      <entry>8</entry>
    </row>
    <row>
      <entry>char</entry>
      <entry>data.b[20]</entry>
      <entry>(read/write DATA : 20 byte)</entry>
    </row>
  </tbody>
  </tgroup>
</table>

<table frame="topbot" id="clientmessage_events_format_only_or_last">
  <?dbfo keep-together="always" ?>
<title>The ClientMessage event's format (only or last)</title>
  <tgroup cols="3" align='left' colsep='0' rowsep='0'>
  <colspec colname="col1" colwidth="1.0*"/>
  <colspec colname="col2" colwidth="1.0*" colsep="1"/>
  <colspec colname="col3" colwidth="3.5*"/>
  <spanspec namest="col1" nameend="col2" spanname="span-horiz" align="center"/>
  <thead>
    <row rowsep='1'>
      <entry spanname="span-horiz" colsep='1'>Structure Member</entry>
      <entry>Contents</entry>
    </row>
  </thead>
  <tbody>
    <row>
      <entry>int</entry>
      <entry>type</entry>
      <entry>ClientMessage</entry>
    </row>
    <row>
      <entry>u_long</entry>
      <entry>serial</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Bool</entry>
      <entry>send_event</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Display</entry>
      <entry>*display</entry>
      <entry>The display to which connects</entry>
    </row>
    <row>
      <entry>Window</entry>
      <entry>window</entry>
      <entry>IMS communication window ID</entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>message_type</entry>
      <entry>XInternAtom(display, "_XIM_PROTOCOL", False)</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>format</entry>
      <entry>8</entry>
    </row>
    <row>
      <entry>char</entry>
      <entry>data.b[20]</entry>
      <entry>(read/write DATA : MAX 20 byte)  (*1)</entry>
    </row>
  </tbody>
  </tgroup>
</table>

<para>
(*1) If the data is smaller than 20 byte, all data other than available data
must be 0.
</para>

<para>
Property
</para>

<para>
In the case of large data, data will be sent via the Window Property
for the efficiency.  There are the following two methods to notify
Property, and transport-version is decided which method is used.
</para>

<itemizedlist>
  <listitem>
    <para>
The XChangeProperty function is used to store data in the client
communication window, and Atom of the stored data is notified to the
IM Server via ClientMessage event.
    </para>
  </listitem>
  <listitem>
    <para>
The XChangeProperty function is used to store data in the client
communication window, and Atom of the stored data is notified to the
IM Server via PropertyNotify event.
    </para>
  </listitem>
</itemizedlist>

<para>
The arguments of the XChangeProperty are as follows:
</para>

<table frame="topbot" id="xchangeproperty_events_format">
  <?dbfo keep-together="always" ?>
<title>The XChangeProperty event's format</title>
  <tgroup cols="3" align='left' colsep='0' rowsep='0'>
  <colspec colname="col1" colwidth="1.0*"/>
  <colspec colname="col2" colwidth="1.0*" colsep="1"/>
  <colspec colname="col3" colwidth="3.5*"/>
  <spanspec namest="col1" nameend="col2" spanname="span-horiz" align="center"/>
  <thead>
    <row rowsep='1'>
      <entry spanname="span-horiz" colsep='1'>Argument</entry>
      <entry>Contents</entry>
    </row>
  </thead>
  <tbody>
    <row>
      <entry>Display</entry>
      <entry>*display</entry>
      <entry>The display to which connects</entry>
    </row>
    <row>
      <entry>Window</entry>
      <entry>window</entry>
      <entry>IMS communication window ID</entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>property</entry>
      <entry>read/write property Atom (*1)</entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>type</entry>
      <entry>XA_STRING  </entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>format</entry>
      <entry>8</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>mode</entry>
      <entry>PropModeAppend</entry>
    </row>
    <row>
      <entry>u_char</entry>
      <entry>*data</entry>
      <entry>read/write DATA</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>nelements</entry>
      <entry>length of DATA</entry>
    </row>
  </tbody>
  </tgroup>
</table>

<para>
The read/write property ATOM allocates the following strings by
<olink targetdoc='libX11' targetptr='XInternAtom'><function>XInternAtom</function></olink>.
</para>

<para>
"_clientXXX"
</para>

<para>
The client changes the property with the mode of PropModeAppend and
the IM Server will read it with the delete mode i.e. (delete = True).
</para>

<para>
If Atom is notified via ClientMessage event, the format of the ClientMessage
is as follows:
</para>

<table frame="topbot" id="clientmessage_events_format_to_send_atom_of_property">
  <?dbfo keep-together="always" ?>
<title>The ClientMessage event's format to send Atom of property</title>
  <tgroup cols="3" align='left' colsep='0' rowsep='0'>
  <colspec colname="col1" colwidth="1.0*"/>
  <colspec colname="col2" colwidth="1.0*" colsep="1"/>
  <colspec colname="col3" colwidth="3.5*"/>
  <spanspec namest="col1" nameend="col2" spanname="span-horiz" align="center"/>
  <thead>
    <row rowsep='1'>
      <entry spanname="span-horiz" colsep='1'>Structure Members</entry>
      <entry>Contents</entry>
    </row>
  </thead>
  <tbody>
    <row>
      <entry>int</entry>
      <entry>type</entry>
      <entry>ClientMessage</entry>
    </row>
    <row>
      <entry>u_long</entry>
      <entry>serial</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Bool</entry>
      <entry>send_event</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Display</entry>
      <entry>*display</entry>
      <entry>The display to which connects</entry>
    </row>
    <row>
      <entry>Window</entry>
      <entry>window</entry>
      <entry>IMS communication window ID</entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>message_type</entry>
      <entry>XInternAtom(display, "_XIM_PROTOCOL", False)</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>format</entry>
      <entry>32</entry>
    </row>
    <row>
      <entry>long</entry>
      <entry>data.l[0]</entry>
      <entry>length of read/write property Atom</entry>
    </row>
    <row>
      <entry>long</entry>
      <entry>data.l[1]</entry>
      <entry>read/write property Atom</entry>
    </row>
  </tbody>
  </tgroup>
</table>

<para>
Format for the data from the IM Server to the Client
</para>

<para>
<!-- .LP -->
<!-- .RS -->
<!-- .B -->
ClientMessage
</para>
<para>
<!-- .LP -->
The format of the ClientMessage is as follows:
</para>



<table frame="topbot" id="clientmessage_events_format_for_first_or_middle">
  <?dbfo keep-together="always" ?>
<title>The ClientMessage event's format (first or middle)</title>
  <tgroup cols="3" align='left' colsep='0' rowsep='0'>
  <colspec colname="col1" colwidth="1.0*"/>
  <colspec colname="col2" colwidth="1.0*" colsep="1"/>
  <colspec colname="col3" colwidth="3.5*"/>
  <spanspec namest="col1" nameend="col2" spanname="span-horiz" align="center"/>
  <thead>
    <row rowsep='1'>
      <entry spanname="span-horiz" colsep='1'>Structure Members</entry>
      <entry>Contents</entry>
    </row>
  </thead>
  <tbody>
    <row>
      <entry>int</entry>
      <entry>type</entry>
      <entry>ClientMessage</entry>
    </row>
    <row>
      <entry>u_long</entry>
      <entry>serial</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Bool</entry>
      <entry>send_event </entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Display</entry>
      <entry>*display</entry>
      <entry>The display to which connects</entry>
    </row>
    <row>
      <entry>Window</entry>
      <entry>window</entry>
      <entry>client communication window ID</entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>message_type</entry>
      <entry>XInternAtom(display, "_XIM_MOREDATA", False)</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>format</entry>
      <entry>8</entry>
    </row>
    <row>
      <entry>char</entry>
      <entry>data.b[20]</entry>
      <entry>(read/write DATA : 20 byte)</entry>
    </row>
  </tbody>
  </tgroup>
</table>


<table frame="topbot" id="clientmessage_events_format_for_only_or_last">
  <?dbfo keep-together="always" ?>
<title>The ClientMessage event's format (only or last)</title>
  <tgroup cols="3" align='left' colsep='0' rowsep='0'>
  <colspec colname="col1" colwidth="1.0*"/>
  <colspec colname="col2" colwidth="1.0*" colsep="1"/>
  <colspec colname="col3" colwidth="3.5*"/>
  <spanspec namest="col1" nameend="col2" spanname="span-horiz" align="center"/>
  <thead>
    <row rowsep='1'>
      <entry spanname="span-horiz" colsep='1'>Structure Members</entry>
      <entry>Contents</entry>
    </row>
  </thead>
  <tbody>
    <row>
      <entry>int</entry>
      <entry>type</entry>
      <entry>ClientMessage</entry>
    </row>
    <row>
      <entry>u_long</entry>
      <entry>serial</entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Bool</entry>
      <entry>send_event </entry>
      <entry>Set by the X Window System</entry>
    </row>
    <row>
      <entry>Display</entry>
      <entry>*display</entry>
      <entry>The display to which connects</entry>
    </row>
    <row>
      <entry>Window</entry>
      <entry>window</entry>
      <entry>client communication window ID</entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>message_type</entry>
      <entry>XInternAtom(display, "_XIM_PROTOCOL", False)</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>format</entry>
      <entry>8</entry>
    </row>
    <row>
      <entry>char</entry>
      <entry>data.b[20]</entry>
      <entry>(read/write DATA : MAX 20 byte) (*1)</entry>
    </row>
  </tbody>
  </tgroup>
</table>

<para>
(*1) If the data size is smaller than 20 bytes, all data other than available
data must be 0.
</para>

<para>
Property
</para>

<para>
In the case of large data, data will be sent via the Window Property
for the efficiency. There are the following two methods to notify
Property, and transport-version is decided which method is used.
</para>

<itemizedlist>
  <listitem>
    <para>
The XChangeProperty function is used to store data in the IMS
communication window, and Atom of the property is sent via the
ClientMessage event.
    </para>
  </listitem>
  <listitem>
    <para>
The XChangeProperty function is used to store data in the IMS
communication window, and Atom of the property is sent via
PropertyNotify event.
    </para>
  </listitem>
</itemizedlist>

<para>
The arguments of the XChangeProperty are as follows:
</para>

<table frame="topbot" id="xchangeproperty_events_format_2">
  <?dbfo keep-together="always" ?>
<title>The XChangeProperty event's format</title>
  <tgroup cols="3" align='left' colsep='0' rowsep='0'>
  <colspec colname="col1" colwidth="1.0*"/>
  <colspec colname="col2" colwidth="1.0*" colsep="1"/>
  <colspec colname="col3" colwidth="3.5*"/>
  <spanspec namest="col1" nameend="col2" spanname="span-horiz" align="center"/>
  <thead>
    <row rowsep='1'>
      <entry spanname="span-horiz" colsep='1'>Argument</entry>
      <entry>Contents</entry>
    </row>
  </thead>
  <tbody>
    <row>
      <entry>Display</entry>
      <entry>*display</entry>
      <entry>The display which to connects</entry>
    </row>
    <row>
      <entry>Window</entry>
      <entry>window</entry>
      <entry>client communication window ID</entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>property</entry>
      <entry>read/write property Atom (*1)</entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>type</entry>
      <entry>XA_STRING</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>format</entry>
      <entry>8</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>mode</entry>
      <entry>PropModeAppend</entry>
    </row>
    <row>
      <entry>u_char</entry>
      <entry>*data</entry>
      <entry>read/write DATA</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>nelements</entry>
      <entry>length of DATA</entry>
    </row>
  </tbody>
  </tgroup>
</table>

<para>
(*1)  The read/write property ATOM allocates some strings, which are not
allocated by the client, by <olink targetdoc='libX11' targetptr='XInternAtom'><function>XInternAtom</function></olink>.
</para>

<para>
The IM Server changes the property with the mode of PropModeAppend and
the client reads it with the delete mode, i.e. (delete = True).
</para>

<para>
If Atom is notified via ClientMessage event, the format of the ClientMessage
is as follows:
</para>


<table frame="topbot" id="clientmessage_events_format_to_send_atom_of_property_2">
  <?dbfo keep-together="always" ?>
<title>The ClientMessage event's format to send Atom of property</title>
  <tgroup cols="3" align='left' colsep='0' rowsep='0'>
  <colspec colname="col1" colwidth="1.0*"/>
  <colspec colname="col2" colwidth="1.0*" colsep='1'/>
  <colspec colname="col3" colwidth="3.5*"/>
  <spanspec namest="col1" nameend="col2" spanname="span-horiz" align="center"/>
  <thead>
    <row rowsep='1'>
      <entry spanname="span-horiz" colsep='1'>Structure Member</entry>
      <entry>Contents</entry>
    </row>
  </thead>
  <tbody>
    <row>
      <entry>int</entry>
      <entry>type</entry>
      <entry>ClientMessage  </entry>
    </row>
    <row>
      <entry>u_long</entry>
      <entry>serial</entry>
      <entry>Set by the X Window System  </entry>
    </row>
    <row>
      <entry>Bool</entry>
      <entry>send_event</entry>
      <entry>Set by the X Window System  </entry>
    </row>
    <row>
      <entry>Display</entry>
      <entry>*display</entry>
      <entry>The display to which connects  </entry>
    </row>
    <row>
      <entry>Window</entry>
      <entry>window</entry>
      <entry>client communication window ID  </entry>
    </row>
    <row>
      <entry>Atom</entry>
      <entry>message_type</entry>
      <entry>XInternAtom(display, "_XIM_PROTOCOL", False)</entry>
    </row>
    <row>
      <entry>int</entry>
      <entry>format</entry>
      <entry>32  </entry>
    </row>
    <row>
      <entry>long</entry>
      <entry>data.l[0]</entry>
      <entry>length of read/write property ATOM  </entry>
    </row>
    <row>
      <entry>long</entry>
      <entry>data.l[1]</entry>
      <entry>read/write property ATOM  </entry>
    </row>
  </tbody>
  </tgroup>
</table>

<para>
Closing Connection
</para>

<para>
If the client disconnect with the IM Server, shutdown function should
free the communication window properties and etc..
</para>
</appendix>
</article>
